For 1990-2009 cars

Table 1: | Heated Seat Module (LH)
Table 2: | LH Lumbar Motor (Buick)
Table 3: | LH Seat Belt Retractor Actuator
Table 4: | LH Seat Recline Motor
Table 5: | LH Seat Switch (Oldsmobile)
Table 6: | LH Seat/Lock Switch (Oldsmobile)
Table 7: | Lumbar Seat Module (C1)
Table 8: | Lumbar Seat Module (C2)
Table 9: | Memory Seat/Mirror Diagnostic Connector
Table 10: | Memory Seat/Mirror Module (MSM) C3
Table 11: | Memory Seat/Mirror Module (C1)
Table 12: | Memory Seat/Mirror Module C2
Table 13: | RH Heated Seat
Table 14: | Heated Seat Module (RH)
Table 15: | RH Seat Belt Retractor Actuator
Table 16: | RH Seat Front Vertical Motor (Oldsmobile)
Table 17: | RH Seat Horizontal Motor (Oldsmobile)
Table 18: | RH Seat Rear Vertical Motor (Oldsmobile)
Table 19: | RH Seat Recline Motor (Oldsmobile)
Table 20: | RH Seat Switch (Oldsmobile)
Table 21: | RH Seat/Lock Switch
Table 22: | LH Seat Front Vertical Position Sensor
Table 23: | LH Seat Horizontal Position Sensor
Table 24: | LH Seat Rear Vertical Position Sensor

#### Heated Seat Module (LH)

Connector Part Information |

• | 12064998

• | 8 Way F Metri-Pack

• | 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 41 | Fused Output -- Ign
B | RED | 742 | Fused Output -- Bat
C | LT BLU | 1462 | Heated Seat Switch Signal
D | BRN | 1463 | Heated Seat Indicator Lamp Feed -- Low Temperature
E | BLK | 150 | Ground
F | DK BLU | 1461 | Heated Seat Indicator Lamp Feed
G | LT BLU/WHT | 181 | Heated Seat Control Module Signal -- Status
H | -- | -- | Not Used

#### LH Lumbar Motor (Buick)

Connector Part Information |

• | 12129155

• | 2 Way M Metri-Pack

• | 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 611 | Power Seat Motor Feed - Driver Lumbar - Out
B | PNK | 610 | Power Seat Motor Feed - Driver Lumbar - In

#### LH Seat Belt Retractor Actuator

Connector Part Information |

• | 12047662

• | 2 Way F Metri-Pack

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1540 | Fused Output - Bat
B | BLK | 155 | Seat Belt Retractor Solenoid Output - Left Front

#### LH Seat Recline Motor

Connector Part Information |

• | 12129081

• | 2 Way F Metri-Pack

• | 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 277 | Power Seat Motor Feed - Driver - Recline - Back
B | LT GRN | 276 | Power Seat Motor Feed - Driver - Recline - Forward

#### LH Seat Switch (Oldsmobile)

Connector Part Information |

• | 12129432

• | 16 Way F Metri-Pack

• | 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 40 | Fused Output - Bat
B | ORN | 40 | Fused Output - Bat
C | GRY | 8 | Instrument Panel Lamp Feed
D | BLK | 150 | Ground
E | LT BLU | 277 | Power Seat Motor Feed - Driver - Recline -Back
F | LT GRN | 276 | Power Seat Motor Feed - Driver - Recline - Forward
G-K | -- | -- | Not Used
L | TAN | 1522 | Power Seat Switch Signal - Horizontal Forward
M | LT GRN | 1523 | Power Seat Switch Signal - Horizontal - Back
N | YEL | 1519 | Power Seat Switch Signal - Rear Vertical Down
P | LT BLU | 1521 | Power Seat Switch Signal - Rear Vertical Down
R | DK GRN | 1518 | Power Seat Switch Signal - Front Vertical Up
S | DK BLU | 1520 | Power Seat Switch Signal - Front Vertical Down

#### LH Seat/Lock Switch (Oldsmobile)

Connector Part Information |

• | 12129429

• | 16 Way F Metri-Pack 280 Series (WHT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | ORN | 40 | Fused Output - Bat
C | GRY | 8 | Instrument Panel Lamp Feed
D | BLK/WHT | 151 | Ground
E | ORN | 614 | Memory Seat Switch Signal - Set
F | WHT | 615 | Memory Seat Switch Signal - Memory 1
G | PPL | 616 | Memory Seat Switch Signal - Memory 2
H | LT BLU | 1462 | Heated Seat Switch Signal
J | DK BLU | 1461 | Heated Seat Indicator Lamp Feed
K | BRN | 1463 | Heated Seat Indicator Lamp Feed - Low Temperature
L | RED | 387 | Power Seat Relay Feed - Coil - Driver Lumbar Up
M | PPL | 385 | Power Seat Relay Feed - Coil - Driver Lumbar - Out
N | YEL | 386 | Power Seat Relay Feed - Coil - Driver Lumbar - Down
P | GRY | 388 | Remote Radio Signal - Right Audio
R | RED/BLK | 780 | Power Door Lock Switch Output - Driver Switch - Lock
S | ORN/BLK | 781 | Power Door Lock Switch Output - Driver Switch - Unlock

#### Lumbar Seat Module (C1)

Connector Part Information |

• | 12092254

• | 6 Way F Metri-Pack

• | 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 2040 | Fused Output (Bat)
B | GRY | 388 | Remote Radio Signal - Right Audio
C | GRY | 758 | Power Seat Relay Feed - Coil - Passenger Lumbar - In
D | PPL | 385 | Power Seat Relay Feed - Coil - Driver Lumbar - Out
E | RED | 756 | Power Seat Relay Feed - Coil - Passenger Lumbar - Up
F | PPL | 759 | Power Seat Relay Feed - Coil - Passenger Lumbar - Out

#### Lumbar Seat Module (C2)

Connector Part Information |

• | 12052856

• | 4 Way F Metri-Pack

• | 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 387 | Power Seat Relay Feed - Coil - Driver Lumbar - Up
B | YEL | 757 | Power Seat Relay Feed - Coil - Passenger Lumbar - Down
C | YEL | 386 | Power Seat Relay Feed - Coil - Driver Lumbar - Down
D | BLK | 150 | Ground

#### Memory Seat/Mirror Diagnostic Connector

Connector Part Information |

• | 12059885

• | 1 Way M Metri-Pack

• | 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL/BLK | 571 | Diagnostic Signal - Memory Seat

#### Memory Seat/Mirror Module (MSM) C3

Connector Part Information |

• | 12064762

• | 6 Way F Metri-Pack

• | 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 81 | Power Mirror Motor Feed - Left Horizontal Motor - Right Direction
B | LT BLU | 82 | Power Mirror Motor Feed - Left Horizontal Motor - Left Direction
C | YEL | 88 | Power Mirror Motor Feed - Left Vertical Motor - Up Direction
D | LT GRN | 89 | Power Mirror Motor Feed - Left Vertical Motor - Down Direction
E | RED/WHT | 881 | Power Mirror Motor Feed - Right Horizontal Motor - Right Direction
F | PPL/WHT | 889 | Power Mirror Motor Feed - Right Vertical Motor - Down Direction

#### Memory Seat/Mirror Module (C1)

Connector Part Information |

• | 12110207

• | 32 Way F Micro-Pack

• | 100 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1 | DK GRN | 784 | Memory Mirror Position Sensor Signal - Left Vertical Motor
C2 | GRY | 786 | Memory Mirror Position Sensor Signal - Left Horizontal Motor
C3 | BRN | 787 | Memory Mirror Position Sensor Signal - Right Vertical Motor
C4 | RED/WHT | 1513 | Power Mirror Switch Signal - Right Horizontal Motor - Right Direction
C5 | LT GRN | 275 | Transmission Mounted Neutral Safety Switch Output - Park
C6 | YEL | 1517 | Power Mirror Switch Signal - Left Vertical Motor - Up Direction
C7 | LT GRN | 1523 | Power Seat Switch Signal - Horizontal Aft
C8 | LT GRN | 1514 | Power Mirror Switch Signal - Left Vertical Motor - Down Direction
C9 | PPL | 616 | Memory Seat Switch Signal - Memory 2
C10 | BLK | 782 | Sensor Return - Memory Seat/Mirror
C11 | DK BLU | 198 | Fused Output - Headlamp - Right
C12 | PNK | 39 | Fused Output - Ign 1
C13 | LT GRN | 276 | Power Seat Motor Feed - Driver - Recline Fore
C14 | DK BLU | 1520 | Power Seat Switch Signal - Front Vertical Down
C15 | LT BLU | 1521 | Power Seat Switch Signal - Rear Vertical Down
C16 | LT BLU | 277 | Power Seat Motor Feed - Driver - Recline Aft
D1 | LT BLU/BLK | 785 | Memory Mirror Position Sensor Signal - Right Horizontal Motor
D2 | GRY | 788 | Memory Mirror Position Sensor Feed - 5 Volt Reference
D3 | TAN | 568 | Memory Seat Position Sensor Signal - Rear Vertical Motor
D4 | DK GRN | 569 | Memory Seat Position Sensor Signal - Horizontal Motor
D5 | WHT | 615 | Memory Seat Switch Signal - Memory 1
D6 | LT BLU | 1516 | Power Mirror Switch Signal - Left Horizontal Motor - Left Direction
D7 | PPL/WHT | 1515 | Power Mirror Switch Signal - Right Vertical Motor - Down Direction
D8 | ORN | 614 | Memory Seat Switch Signal - Set
D9 | BRN/WHT | 557 | Memory Seat Position Sensor Signal - Front Vertical Motor
D10 (Buick) | -- | -- | Not Used
D11 | WHT | 1512 | Power Mirror Switch Signal - Left Horizontal Motor - Right Direction
D12 | YEL/BLK | 571 | Diagnostic Signal - Memory Seat
D13 | LT GRN | 24 | Back-up Lamp Feed
D14 | TAN | 1522 | Power Seat Switch Signal - Horizontal Fore
D15 | DK GRN | 1518 | Power Seat Switch Signal - Front Vertical Up
D16 | YEL | 1519 | Power Seat Switch Signal - Rear Vertical Up

#### Memory Seat/Mirror Module C2

Connector Part Information |

• | 12064749

• | 2 Way F Metri-Pack

• | 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1340 | Fused Output - Bat
B | BLK | 150 | Ground

#### RH Heated Seat

Connector Part Information |

• | 12059800

• | 5 Way F Metri-Pack

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | LT BLU/BLK | 1505 | Heated Seat Switch Signal - Passenger
C | DK BLU/WHT | 1504 | Heated Seat Indicator Lamp Feed - Passenger
D | BRN/WHT | 1506 | Heated Seat Indicator Lamp Feed - Passenger - Low Temperature
E | BLK/WHT | 151 | Ground

#### Heated Seat Module (RH)

Connector Part Information |

• | 12064998

• | 8 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 41 | Fused Output -- Ign
B | RED | 742 | Fused Output -- Bat
C | LT BLU/BLK | 1505 | Heated Seat Switch Signal -- Passenger
D | BRN/WHT | 1506 | Heated Seat Indicator Lamp Feed -- Passenger -- Low Temperature
E | BLK | 151 | Ground
F | DK BLU/WHT | 1504 | Heated Seat Indicator Lamp Feed -- Passenger
G | LT BLU/WHT | 181 | Heated Seat Control Module Signal -- Status
H | -- | -- | Not Used

#### RH Seat Belt Retractor Actuator

Connector Part Information |

• | 12047662

• | 2 Way F Metri-Pack

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1540 | Fused Output - Bat
B | YEL | 528 | Seat Belt Retractor Solenoid Output - Right Front

#### RH Seat Front Vertical Motor (Oldsmobile)

Connector Part Information |

• | 12020556

• | 2 Way F Metri-Pack

• | 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 298 | Power Seat Motor Feed - Passenger - Front Vertical - Down
B | DK GRN | 297 | Power Seat Motor Feed - Passenger - Front Vertical - Up

#### RH Seat Horizontal Motor (Oldsmobile)

Connector Part Information |

• | 12052110

• | 2 Way F Metri-Pack

• | 480 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 296 | Power Seat Motor Feed - Passenger - Horizontal - Forward
B | LT GRN | 290 | Power Seat Motor Feed - Passenger - Horizontal - Back

#### RH Seat Rear Vertical Motor (Oldsmobile)

Connector Part Information |

• | 12052109

• | 2 Way F Metri-Pack

• | 480 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 288 | Power Seat Motor Feed - Passenger - Rear Vertical - Up
B | LT BLU | 289 | Power Seat Motor Feed - Passenger - Rear Vertical Down

#### RH Seat Recline Motor (Oldsmobile)

Connector Part Information |

• | 12129081

• | 2 Way F Metri-Pack

• | 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 77 | Power Seat Motor Feed - Passenger - Recline - Back
B | DK GRN | 76 | Power Seat Motor Feed - Passenger - Recline - Forward

#### RH Seat Switch (Oldsmobile)

Connector Part Information |

• | 12129432

• | 16 Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1340 | Fused Output - Bat
B | -- | -- | Not Used
C | GRY | 8 | Instrument Panel Lamp Feed
D | BLK/WHT | 151 | Ground
E | DK BLU | 77 | Power Seat Motor Feed-Passenger- Recline - Back
F | DK GRN | 76 | Power Seat Motor Feed-Passenger- Recline - Forward
G-K | -- | -- | Not Used
L | TAN | 296 | Power Seat Motor Feed-Passenger- Horizontal - Forward
M | LT GRN | 290 | Power Seat Motor Feed-Passenger- Horizontal - Back
N | YEL | 288 | Power Seat Motor Feed-Passenger- Rear Vertical Up
P | LT BLU | 289 | Power Seat Motor Feed-Passenger- Rear Vertical Down
R | DK GRN | 297 | Power Seat Motor Feed-Passenger- Front Vertical Up
S | DK BLU | 298 | Power Seat Motor Feed-Passenger- Front Vertical Down

#### RH Seat/Lock Switch

Connector Part Information |

• | 12129429

• | 16 Way F Metri-Pack 280 Series (WHT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | ORN | 40 | Fused Output-Bat
C | GRY | 8 | Instrument Panel Lamp Feed
D | BLK/WHT | 151 | Ground
E-G | -- | -- | Not Used
H | LT BLU/BLK | 1505 | Heated Seat Switch Signal-Passenger
J | DK BLU/WHT | 1504 | Heated Seat Indicator Lamp Feed-Passenger
K | BRN/WHT | 1506 | Heated Seat Indicator Lamp Feed-Passenger- Low Temperature
L | RED | 756 | Power Seat Relay Feed-Coil- Passenger Lumbar-Up
M | PPL | 759 | Power Seat Relay Feed-Coil- Passenger Lumbar-Out
N | YEL | 757 | Power Seat Relay Feed-Coil- Passenger Lumbar-Down
P | GRY | 758 | Power Seat Relay Feed-Coil- Passenger Lumbar-In
R | RED/BLK | 780 | Power Door Lock Switch Output-Driver Switch-Lock
S | ORN/BLK | 781 | Power Door Lock Switch Output-Driver Switch-Unlock

#### LH Seat Front Vertical Position Sensor

Connector Part Information |

• | 12059584

• | 3 Way F Metri-Pack

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
B | GRY | 788 | Memory Mirror Position Sensor Feed - 5 Volt Reference
C | BRN/WHT | 557 | Memory Seat Position Sensor Signal - Front Vertical Motor
D | BLK | 782 | Sensor Return - Memory Seat/Mirror

#### LH Seat Horizontal Position Sensor

Connector Part Information |

• | 12059583

• | 3 Way F Metri-Pack

• | 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 788 | Memory Mirror Position Sensor Feed - 5 Volt Reference
C | DK GRN | 569 | Memory Seat Position Sensor Signal - Horizontal Motor
D | BLK | 782 | Sensor Return - Memory Seat/Mirror

#### LH Seat Rear Vertical Position Sensor

Connector Part Information |

• | 12059582

• | 3 Way F Metri-Pack

• | 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 782 | Sensor Return - Memory Seat/Mirror
B | TAN | 568 | Memory Seat Position Sensor Signal - Rear Vertical Motor
D | GRY | 788 | Memory Mirror Position Sensor Feed - 5 Volt Reference