For 1990-2009 cars

# POWER STEERING PUMP REMOVAL CORRECTION-1984 SERVICE MANUAL

#### VEHICLES AFFECTED: 1984 'G', 'B', 'D', and 'E' Series Vehicles Equipped With LV2 or LF9 Engines

When removing the power steering pump on a 1984 V-8 engine, it is not necessary to remove the fan and clutch assembly as described on page 3B7-3 of the 1984 Chassis Service Manual. Please correct your manual accordingly.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.