For 1990-2009 cars

# EXTENDED CRANK TIME (NEW PART)

#### MODELS AFFECTED: SOME 1989 AND EARLY BUILT 1990 BUICK LESABRES, ELECTRAS, RIVIERAS AND REATTAS EQUIPPED WITH THE 3800 ENGINE (VIN CODE C)

Some 1989 through early built 1990 LeSabres, Electras, Rivieras and Reattas equipped with the 3800 engine (VIN Code C), may exhibit a condition of a cold engine extended crank, but if the ignition key is cycled, the engine will start.

If this condition is experienced on a vehicle with good fuel pressure and the basic engine controls and systems are performing properly, it may be necessary to install a new service Mem-Cal with a recalibrated fuel multiplier ratio during cranking.

Service Mem-Cals are currently available from GMSPO.

#### IMPORTANT: The new calibration Mem-Cals are currently being used in production. Verify if this Mem-Cal is already installed by the Scanner I.D.

Axle Option *Scanner Mem-Cal Code Located I.D. If this Service Model Axle on Service Mem-Cal is Part Year Application Ratio Pts.I.D. Label Installed Number --- ----------- ----- -------------- --------- ------ 89/90 FED LeSab./Elec 2.84 F17 8094 16148060 89/90 CAL LeSab./Elec 2.84 F17 7994 16148005 89/90 FED LeSab./Elec. 2.97 F79 8004 16148006 89/90 CAL LeSab./Elec. 2.97 F79 8014 16148007 89 FED Riv. 2.84 F17 1074 16141292 89 CAL Riv. 2.84 F17 1084 16141296 89 FED Riv./Reatta 2.97 F79 1094 16141300 89 CAL Riv./Reatta 2.97 F79 1104 16141305 90 FED Riv. 2.97 F79 8084 16148016 90 CAL Riv. 2.97 F79 7984 16148003 90 FED Reatta 2.97 F79 8064 16148013 90 CAL Reatta 2.97 F79 8074 16148015

WARRANTY INFORMATION

Labor Operation Number: T5191 Labor Time: .5 Hours Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.