For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Handle Bezel Screw (Buick) | 1 N·m | 9 lb in
Door Hinge Bolts | 48 N·m | 35 lb ft
Door Trim Hanger Bracket (Oldsmobile) Front Screw | 10 N·m | 89 lb in
Door Trim Hanger Bracket (Oldsmobile) Rear Screw | 3 N·m | 27 lb in
Handle Bezel to Front Door (Oldsmobile) | 3 N·m | 27 lb in
Handle Bezel to Rear Door | 3 N·m | 27 lb in
Lock Assembly to Door Retaining Screws | 7 N·m | 62 lb in
Lower Front Door Panel Screws (Oldsmobile) | 1.9 N·m | 17 lb in
Lower Rear Door Panel Screws (Oldsmobile) | 1.8 N·m | 16 lb in
Pull Handle Screws (Buick) | 7 N·m | 62 lb in
Rear Door Outside Handle | 7 N·m | 62 lb in
Striker Bolts | 25 N·m | 18 lb ft
Upper Trim Panel Screws (Buick) | 1 N·m | 9 lb in
Window Clamp Glass Retaining Bolts | 9 N·m | 80 lb in