For 1990-2009 cars

Table 1: | Body Control Module (MALL) C1
Table 2: | Body Control Module (MALL) C2

#### Body Control Module (MALL) C1

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pak 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 694 | Power Door Lock Motor Feed - Driver Door Unlock
B | -- | -- | Not Used
C | GRY | 295 | Power Door Lock Motor Feed - Lock
D | BLK | 150 | Ground
E | ORN | 1732 | Electronic Control Unit Output - 12 volt - Indavertent Load Control
F | WHT | 156 | Courtesy Lamp - Output
G | ORN | 640 | Fuse Output - Battery
H | ORN | 1540 | Fuse Output - Battery

#### Body Control Module (MALL) C2

Connector Part Information |

• | 12110207

• | 32-Way F Micro-Pak

• | 100 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1 | BLK | 155 | Seat Belt Retractor Solenoid Output - Left Front
C2 | DK BLU | 1393 | Interior Lamp Relay Output - Coil
C3 (Buick) | YEL | 528 | Seat Belt Retractor Solenoid Output - Right Front
C3 (Oldsmobile) | DK BLU | 49 | Door Lock Actuator Signal - Driver
C4 | LT GRN/BLK | 394 | Door Handle Switch Signal - Left Front
C5 | -- | -- | Not Used
C6 | ORN/BLK | 781 | Power Door Lock Switch Output - Driver Switch - Unlock
C7 | LT BLU | 195 | Power Door Lock Relay Feed - Lock Coil
C8-C11 | -- | -- | Not Used
C12 (Buick) | PPL | 16 | Turn Signal Flasher Output
C12 (Oldsmobile | -- | -- | Not Used
C13 | PNK | 39 | Fuse Output (Ignition 1)
C14 | -- | -- | Not Used
C15 | DK GRN/WHT | 817 | Vehicle Speed Signal - 4000 Pulses Per Mile
C16 | -- | -- | Not Used
D1 | BLK/WHT | 238 | Seat Belt Switch Signal
D2 | DK BLU/WHT | 653 | Chime Module Signal - Bit 1
D3 (Buick) | TAN/WHT | 33 | Brake Warning Indicator Lamp Output
D3 (Oldsmobile | LT GRN | 1845 | Multi-Function Chime Control Signal
D4 | -- | -- | Not Used
D5 (Buick) | PPL/WHT | 549 | Headlamp Switch Signal - Headlamps OFF
D5 (Oldsmobile) | LT BLU | 1785 | Park Lamp Switch Output - Park Lamps OFF
D6-11 | -- | -- | Not Used
D12 | YEL | 234 | Seat Belt Indicator Lamp Output
D13-16 | -- | -- | Not Used