For 1990-2009 cars

# CLIMATE CONTROL TEMP. BUTTON INOPERATIVE

CLIMATE CONTROL HEAD "WARM" OR "COLD" BUTTON INOPERATIVE

#### Vehicles Affected: 1988 TORONADO -----------------

Some 1988 Toronados built before VIN breakpoint number 303500 may experience an inoperative "WARM" or "COLD" button. If diagnosis of this problem leads to the ECC head, use P/N 1228821 for replacement.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.