For 1990-2009 cars

## Cornering Lamp Replacement Oldsmobile

The cornering lamps (1) are an integral part of the front sidemarker lamps. Refer to Side Marker Lamp Replacement .

## Cornering Lamp Replacement Buick

### Removal Procedure

1. Remove the screw (3) from the cornering lamp (2).
2. Remove the cornering lamp (2) from the headlamp housing.
3. Turn the socket in a counterclockwise direction in order to remove the socket (1) from the lamp assembly.
4. Remove the bulb from the socket (1).

### Installation Procedure

1. Install the bulb to the socket (1).
2. Install the socket (1) to the lamp assembly.
3. Install the cornering lamp (2) to the headlamp assembly.

Align the retaining pin in the notch.

4. Install the screw (3) into the cornering lamp (2).