For 1990-2009 cars

### Compact Disc (CD) Skip

The compact disc (CD) player has been designed with a shock absorbing system. Only under extreme operating temperatures or sever shock or vibration should the compact disc player skip or mute. If the customer travels a abnormally rough road a skip condition may be normal. Test drive the vehicle on a normal road with a known good CD, if the condition is still present, replace the compact disc (CD) player.

### Compact Disc (CD) Player Error or Ejects

• | Check the CD for scratches or smudges and clean it if necessary.

• | Check that the CDs and or CD magazine are being loaded correctly.

• | Check that the compact disc player door is closed.

• | During periods of high humidity the CD or the CD player lens may become temporarily fogged, allow the CD player and CDs warm up to dissipate the moisture.