For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Press the door LOCK button on the transmitter. | All of the doors lock. | Door Lock Inoperative with Transmitter - All
2 | Press the door UNLOCK button on the transmitter. | The left front door unlocks. | Door Unlock Inoperative with Transmitter - Left Side Front
3 | Press the door UNLOCK button on the transmitter twice within 4 seconds. | All of the doors unlock. | Door Lock Inoperative with Transmitter - All
4 | Press the rear compartment release button on the transmitter. | The rear compartment lid opens. | Rear Release Inoperative with Transmitter
5 | Press the panic button on the transmitter. |

• | The horns sound.

• | The lights flash.

Panic Mode Inoperative

6 | Press any button on the transmitter. | The selected function actuates. | Keyless Entry System Inoperative
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.