For 1990-2009 cars

## Fastener Tightening Specifications Buick

Application | Specification
--- | ---
Metric | English
Ashtray Fasteners | 1.9 N·m | 17 lb in
Console to Floor Pan Fasteners | 10 N·m | 89 lb in
Console to Instrument Panel Carrier Fasteners | 1.9 N·m | 17 lb in
Console to Shifter Bracket Fasteners | 10 N·m | 89 lb in
Console Trim Plate Fasteners | 1.9 N·m | 17 lb in
Instrument Panel Cluster to Instrument Panel Fasteners | 1.6 N·m | 14 lb in
Instrument Panel Center Air Outlet Fastener | 2 N·m | 18 lb in
Instrument Panel Carrier Center Support Bracket Fasteners | 10 N·m | 89 lb in
Instrument Panel Carrier Left Side Outer Bracket Fastener | 1.9 N·m | 17 lb in
Instrument Panel Carrier Right Side Outer Bracket Fasteners | 9 N·m | 80 lb in
Instrument Panel Carrier to Dash Panel L-Bracket Fasteners | 1.9 N·m | 17 lb in
Instrument Panel Compartment to Instrument Panel Fasteners | 1.9 N·m | 17 lb in
Instrument Panel Side Trim Panel Fastener | 1.9 N·m | 17 lb in
Instrument Panel Upper Trim Pad Fasteners | 1.9 N·m | 17 lb in
Knee Bolster Deflector Fasteners | 20 N·m | 15 lb ft
Knee Bolster Fasteners | 9 N·m | 80 lb in
Sound Insulator to Dash Panel Fasteners | 1.9 N·m | 17 lb in

## Fastener Tightening Specifications Oldsmobile

Application | Specification
--- | ---
Metric | English
Console Compartment Bin Fasteners | 1.3 N·m | 15 lb in
Console to Floor Pan Fasteners | 9 N·m | 80 lb in
Console to Instrument Panel Fasteners | 1.9 N·m | 17 lb in
Console to Shifter Bracket Fasteners | 9 N·m | 80 lb in
Console Trim Plate Fasteners | 1.9 N·m | 17 lb in
Instrument Panel Carrier to Center Support Bracket Fasteners | 10 N·m | 89 lb in
Instrument Panel Carrier to Outer Support Bracket Fasteners | 10 N·m | 89 lb in
Instrument Panel Carrier to Upper L-Bracket Fastener | 1.9 N·m | 17 lb in
Instrument Panel Storage Compartment to Instrument Panel Fasteners | 1.9 N·m | 17 lb in
Instrument Panel Upper Trim Pad Fasteners | 1.9 N·m | 17 lb in
Knee Bolster Fasteners | 9 N·m | 80 lb in
Knee Bolster Deflector Fasteners | 20 N·m | 15 lb ft
Knee Bolster Reinforcement Fasteners | 9 N·m | 80 lb in
Sound Insulator to Dash Panel Screws/Nuts | 1.9 N·m | 17 lb in