For 1990-2009 cars

# DIESEL ENGINE INJECTION PUMP STANADYNE PUMP REPAIR PARTS

THE FOLLOWING LISTS STANADYNE DIESEL ENGINE INJECTION PUMP SERVICE REPAIR PARTS THAT ARE NOW AVAILABLE FROM WDDGM.

STANADYNE WDDGM P/N P/N PART NAME

22935 14063880 RING FLEX RET. 22840 14067401 SOL. ASM. COLD ADV. 22702 14067403 SEAL ADV. PLUNGER 22963 14067404 KIT GASKET REBUILD 23265 14067405 RET.ASM. GOV. WT. 21284 14067406 PIN VAC. MOD'LE DR. 21247 14067407 SEAL CONNECTOR 20113 14067408 SEAL ADV. PISTON HOLE PLUG 17438 14067409 SEAL THROTTLE SHAFT 12766 14067410 SEAL ADV. SER. HOLE PLG. 22149 14067411 KIT SHUT DOWN COIL ARM & SOL.FRAME ASM. 12054 14067413 GASKET CONTROL CVR. 11304 14067414 SEAL AYDRAULIC HEAD 11507 14067415 SEAL HEAD LOCATING SCREW 12764 14067416 SEAL ADV. PISTON HOLE PLUG 22503 14067417 GASKET TIMING WINDOW CVR. 22399 14067418 SEAL ADV. PISTON HOLE 22937 14067419 "O" RING DRIVE SHAFT RET. 20526 14067421 SEAL TRANSFER PUMP 10574 14067423 GASKET TIMING LINE CVR. 13622 22504915 SEAL PILOT TUBE 15892 22507974 SEAL PRESS TAP PLUG & GUIDE ST'D. 10464 561888 SEAL PRESS TAP PLUG 12259 561887 SCREW HS'G PRESS TAP 22601 22507975 SCREW HS'G PRESS TAP 23530 22518470 CONN. ASM. RET. LINE 22109 22517238 CONN. ASM. 23509 14067402 GASKET, TIMING LINE CVR.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.