For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | Under rear seat lower cushion | -- | --
Battery Thermistor | Under rear seat, attached to positive battery cable | 8A-201-37 Fig. 70 | --
Generator | Top RH side of engine | -- | --
Engine Compartment MAXI® Fuse Block | RH front corner of engine compartment | 8A-201-3 Fig. 8 | --
Engine Compartment Power Distribution Center | RH front of engine compartment | 8A-201-3 Fig. 8 | 11-5
I/P Fuse Block | Behind LH side of passenger compartment, attached to door hinge pillar | 8A-201-22 Fig. 42 | 11-0
Instrument Panel Cluster | LH side of I/P | -- | 81-0
Ignition Switch | RH side of steering column | 8A-201-27 Fig. 51 | --
PASS-Key® II Decoder Module | Behind RH side of I/P | 8A-201-30 Fig. 57 | 8A-202-51
RH MAXI® Fuse Block | RH rear of engine compartment, near P101 | 8A-201-12 Fig. 23 | --
RH Rear Power Distribution Center | Under rear seat | -- | --
RH Rear Power Distribution Center Fuse Block #1 | Under rear seat, on LH side | 8A-20 Fig. 711-71 | 11-2
RH Rear Power Distribution Center Fuse Block #2 | Under rear seat, on LH side | 8A-201-71 Fig. 71 | 11-2
Starter Enable Relay | Behind LH side of I/P, on bracket left of steering column | 8A-201-25 Fig. 47 | 19-0
Starter Motor (Buick) | Front of engine, lower LH | 8A-201-8 Fig. 17 | --
Starter Motor (Oldsmobile) | Top of engine under intake manifold | 8A-201-8 Fig. 17 | --
Starter Solenoid | Lower LH front of engine, above starter motor | 8A-201-13 Fig. 25 | --
C101 (78 cavities) | Center rear of engine compartment | 8A-201-7 Fig. 15 | 8A-202-1
C102 (30 cavities) | Center rear of engine compartment, near wiper motor module | 8A-201-7 Fig. 15 | 8A-202-5
C131 (Oldsmobile) | On starter solenoid | 8A-20 Fig. 251-13 | --
C202 (48 cavities) | Behind I/P, at base of steering column | 8A-201-25 Fig. 47,47 | 8A-202-11
G301 | Under rear seat, RH side of battery | 8A-201-37 Fig. 70 | --
P100 | LH rear on engine compartment, behind strut tower | 8A-201-6 Fig. 14 | --
P107 | RH rear of engine compartment, next to strut tower | 8A-201-2 Fig. 5 | --
P108 | RH rear of engine compartment, next to strut tower | 8A-201-31 Fig. 59 | --
S223 | Body harn, approx. 21.5 cm from P100 | 8A-201-22 Fig. 42 | --
S347 | Body harness, approx. 25.5 cm from G302 | 8A-201-34 Fig. 65 | --