For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Engine Oil Cooler Line Fittings (VIN C) | 14 N·m | 10 lb ft
Upper Tie Bar | 10 N·m | 89 lb in
Thermostat Housing Bolts | 10 N·m | 89 lb in
Transaxle Oil Cooler Line Fittings (VIN 1) | 27 N·m | 20 lb ft
Transaxle Oil Cooler Line Fittings (VIN C) | 18 N·m | 13 lb ft
Water Pump (VIN C) | 100 N·m | 74 lb ft
Water Pump Cover | 10 N·m | 89 lb in
Water Pump Housing Bolts (VIN C) | 10 N·m | 89 lb in
Water Pump Mounting Bolts (Long) (VIN 1) | 30 N·m | 22 lb ft
Water Pump Mounting Bolts (Short) (VIN 1) | 15 N·m | 11 lb ft