For 1990-2009 cars

#### Engine Component View -- Vin 1

(1) | Exhaust Gas Recirculation (EGR) Valve
(2) | Idle Air Control (IAC) Valve
(3) | Mass Air Flow (MAF) Sensor
(4) | Throttle Position (TP) Sensor
(5) | Bypass Valve Actuator
(6) | Boost Control Solenoid
(7) | Ignition Control Module
(8) | Crankshaft Position (CKP) Sensor
(9) | Camshaft Position (CMP) Sensor
(10) | EVAP Canister Purge Valve
(11) | Heated Oxygen Sensor 1 (HO2S 1)
(12) | Manifold Absolute Pressure (MAP) Sensor
(13) | PCV Valve

#### Engine Component View Vin K

(1) | Exhaust Gas Recirculation (EGR) Valve
(2) | Idle Air Control (IAC) Valve
(3) | Mass Air Flow (MAF) Sensor
(4) | Throttle Position (TP) Sensor
(5) | Engine Oil Level Switch
(6) | Ignition Control Module
(7) | Crankshaft Position (CKP) Sensor
(8) | Camshaft Position (CMP) Sensor
(9) | EVAP Canister Purge Valve
(10) | PCV Valve
(11) | Heated Oxygen Sensor 1 (HO2S 1)
(12) | Manifold Absolute Pressure (MAP) Sensor

#### Cell 20 -- Component Location Table VIN 1 and K

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
A/C Compressor Clutch | Lower RH front of engine compartment | 8A-201-7 Fig 16 | -- | --
A/C Compressor Clutch Diode | Lower RH front of engine compartment, near A/C compressor conn | 8A-201-7 Fig 16 | -- | --
A/C Pressure Switch | Lower RH front of engine, attached to A/C compressor | 8-Engine Controls | -- | --
Bank #1 Knock Sensor | Lower center front of engine, below exhaust manifold | 8-Engine Controls | 8-Engine controls | --
Bank #2 Knock Sensor | Lower center back of engine, below exhaust manifold | 8-Engine Controls | 8-Engine Controls | --
Body Control Module (BCM) | LH front of passenger compartment, under I/P | 8A-201-25 Fig 47 | 8A-202-51 | --
Boost Control Solenoid | Top of engine, attached to fuel rail | 8-Engine Controls | -- | --
Brake Switch | Behind LH side of I/P, on brake pedal support brace | 8A-201-28 Fig 52 | 8A-202-35 | 4.634
Camshaft Position (CMP) Sensor | RH front of engine, above crankshaft pulley | 8-Engine Controls | -- | --
Crankshaft Position (CKP) Sensor | RH front of engine, forward of the crankshaft pulley | 8-Engine Controls | -- | --
Cruise Control Module | LH rear of engine compartment, center front of dash | 8A-201-7 Fig 15 | -- | --
Data Link Connector (DLC) | Under LH side of I/P, behind sliding door in sound insulator | 8A-201-25 Fig 26 | 8A-202-36 | --
Electronic Brake (and Traction) Control (EBCM/EBTCM) Module | LH side of engine compartment, attached to left strut tower | 8A-201-6 Fig 13 | 8A-202-32 | --
Engine Compartment Power Distribution Center MaxiFuse™Block | RH front of engine compartment, on frame rail | 8A-201-3 Fig 8 | 8A-19-0 | --
Engine Compartment Power Distribution Center Relay Block #1 | RH front of engine compartment, on frame rail | 8A-201-3 Fig 8 | 8A-19-0 | --
Engine Compartment Power Distribution Center Relay Block #2 | RH front of engine compartment, on frame rail | 8A-201-3 Fig 8 | 8A-19-0 | --
Engine Coolant Temperature Sensor | Top LH side of engine, below thermostat housing | 8-Engine Controls | -- | --
Engine Oil Level Switch | Lower front of engine, on oil pan | 8-Engine Controls | -- | --
Engine Oil Pressure Switch | Lower RH rear of engine, below power steering reservoir | 8-Engine Controls | -- | --
Evaporative Emissions (EVAP) Purge Solenoid Valve (VIN 1) | Top RH rear of engine, above valve cover | 8-Engine Controls | -- | --
Evaporative Emissions (EVAP) Purge Solenoid Valve (VIN K) | Top RH rear of engine, above valve cover | 8-Engine Controls | -- | --
Evaporative Emissions (EVAP) Purge Vacuum Switch (VIN K) | Top RH rear of engine, above valve cover | 8-Engine Controls | -- | --
Evaporative Emissions (EVAP) Purge Vacuum Switch (VIN 1) | Top RH rear of engine, above valve cover | 8-Engine Controls | -- | --
Exhaust Gas Recirculation (EGR) Valve | Top LH side of engine, rear of throttle body assembly | 8-Engine Controls | -- | --
Fuel Injectors | Top of engine, below fuel rail | 8-Engine Controls | -- | --
Fuel Level Sender | In top of fuel tank | 8A-201-21 Fig 39 | 8A-202-39 |
Fuel Pump Control Module | LH side of rear compartment, rear of wheelhouse | 8-Engine Controls | -- | --
Heated Oxygen Sensor 1 (HO2S 1) | Rear of engine, in exhaust mainfold | 8-Engine Controls | -- | --
Heated Oxygen Sensor 2 (HO2S 2) | Rear of catalytic converter | 8-Engine Controls | -- | --
HVAC Programmer | Behind RH side of I/P, left of kick panel | 8A-201-30 Fig 56 | 8A-202-43 | --
I/P Fuse Block | LH front of passenger compartment, on end of I/P | 8A-201-22 Fig 42 | 8A-11-0 | 2.483
Idle Air Control (IAC) Valve | LH top of engine, attached to throttle body assembly | 8-Engine Controls | -- | --
Ignition Control Module (ICM) | RH top front of engine, below ignition coils | 8-Engine Controls | 8-Engine Controls | --
Intake Air Temperature (IAT) Sensor | LH side of engine compartment, attached to Air Intake Tube | 8-Engine Controls | -- | --
LH Rear Power Distribution Center Relay Block #3 | Under rear seat, LH side of battery compartment | 8A-201-38 Fig 71 | 8A-10-0 | --
Low speed Cooling Fan Relay | Center rear of engine compartment, left of Windshield Wiper Motor | 8A-201-7 Fig 15 | 8A-19-0 | --
Magna Steer™ Module | LH side of I/P, on bracket left of Steering Column | 8A-201-30 Fig 56 | 8A-202-50 | --
Mainfold Absolute Pressure (MAP) Sensor | Top LH rear of Engine, above Valve Cover | 8-Engine Controls | -- | --
Mass Air Flow (MAF) Sensor | Top LH side of Engine, on Throttle Body Assembly | 8-Engine Controls | -- | --
PASS Key ™II Module | Behind lower RH side of I/P, left of kick panel | 8A-201-30 Fig 57 | 8A-202-64 | --
Powertrain Control Module (PCM) | Behind lower RH of I/P, above kick panel | 8A-201-31 Fig 58 | -- | 3.670
Primary Cooling Fan Diode | RH front of engine compartment, below Secondary Cooling Fan | 8A-201-0 Fig 1 | -- | --
Primary Cooling Fan Motor | LH front of engine compartment | 8A-201-0 Fig 1 | -- | --
Rear MaxiFuse™ Block #2 | Under rear seat, LH side of battery compartment | 8A-201-37 Fig 71 | 8A-10-0 | 2.483
RH Rear Power Distribution Center Fuse Block #1 | Under rear seat, LH side of battery compartment | 8A-201-37 Fig 71 | 8A-11-0 | 2.483
Secondary Cooling Fan Motor | RH front of engine compartment | 8A-201-0 Fig 1 | -- | --
Throttle Position (TP) Sensor | Top LH side of engine, attached to throttle body assembly | 8-Engine Controls | -- | --
Transaxle Range (TR) Switch | LH center of engine compartment, on transaxle | 8-Engine Controls | 8A-202-57 | --
Vehicle Speed Sensor (VSS) | Lower RH rear of engine, below power steering reservoir, attached to transaxle | 8-Engine Controls | -- | 3.682
C100 | LH front of engine, below thermostat housing | 8A-201-16 Fig 29 | 8A-202-0 | --
C101 | Center rear of engine compartment, near bulkhead | 8A-201-7 Fig 15 | 8A-202-1 | --
C102 | Center rear of engine compartment, near windshield wiper motor | 8A-201-7 Fig 15 | --8A-202-5 | --
C107 | RH front of engine, left of ignition control module | 8A-201-12 Fig 22 | 8A-202-6 | --
C111 | RH rear of engine, below power steering reservoir | 8A-201-10 Fig 20 | -- | --
C129 | LH rear of engine, on transaxle | 201-13-26 | -- | --
C202 | Below LH side of I/P, base of steering column | 8A-01-26 Fig 47 | 8A-202-11 | --
G100 | RH front of engine, under ignition control module | 8A-201-12 Fig 22 | -- | --
G101 | Lower RH rear of engine, below power steering reservoir | 201-26-49 | -- | --
G103 | RH side of engine compartment, on lower rail | 8a-201-2 Fig 5 | -- | --
G201 | RH front of passenger compartment, under kick panel trim | 8A-201-31 Fig 59 | -- | --
G202 | LH front of passenger compartment, under kick panel trim | 8A-201-22 Fig 42 | -- | --
G302 | LH rear of passenger compartment, under rear seat | 8A-201-38 Fig 72 | -- | --
P100 | LH rear of engine compartment, behind strut tower | 8A-201-6 Fig 14 | -- | --
P107 | RH rear of engine compartment, near strut tower | 8A-201-2 Fig 5 | -- | --
S100 | Engine harn, approx 6 cm from washer pump conn | 8A-201-2 Fig 5 | -- | --
S104 | Engine harn, approx 25 cm from engine compartment power distribution center | 8A-201-2 Fig 5 | -- | --
S105 | Engine harn, approx 20 cm from A/C compressor clutch | 8A-201-19 Fig 36 | -- | --
S106 | Engine harn, approx 13 cm from C101 | 8A-201-16 Fig 30 | -- | --
S108 | Engine harn, approx 20 cm from A/C compressor clutch | 8A-201-19 Fig 36 | -- | --
S114 | Engine harn, approx 10 cm from C106 | 8A-201-16 Fig 30 | -- | --
S115 | Body harn, approx 12 cm from washer pump motor | 8A-201-2 Fig 5 | -- | --
S116 | Body harn, approx 15.5 cm from P107 | 8A-201-2 Fig 5 | -- | --
S126 | Engine harn, approx 6 cm from C101 | 8A-201-15 Fig 27 | -- | --
S129 | Engine harn, approx 12 cm from C101 | 8A-201-14 Fig 26 | -- | --
S130 | Body harn, approx 38.5 cm from C103 | 8A-201-2 Fig 5 | -- | --
S131(VIN 1) | Engine harn, approx 13 cm from C101 | 8A-201-15 Fig 27 | -- | --
S131 (VIN K) | Engine harn, approx 20 cm from C101 | 8a-201-13 Fig 28 | -- | --
S135 | Ignition control module harn, approx 26.5 cm from ignition control module | 8A-201-11 Fig 21 | -- | --
S136 | Ignition Control Module harn, approx 20 cm from ignition control module | 8A-201-11 Fig 21 | -- | --
S141 | Body harn, approx 5.5 cm from LH engine cooling fan | 8A-201-0 Fig 1 | -- | --
S143 | Engine harn, approx 5.5 cm from RH engine cooling fan | 8A-201-0 Fig 1 | -- | --
S154 | Engine harn, approx 8 cm from idle air control valve | 8A-201-14 Fig 26 | -- | --
S155 | Engine harn, approx 6 cm from idle air control valve | 8A-201-14 Fig 26 | -- | --
S160 | Engine harn, approx 8 cm from fuel injector #5 | 8A-201-13 Fig 23 | -- | --
S209 | Body harn, approx 13 cm from turn signal flasher | 8A-201-29 Fig 54 | -- | --
S211 | Body harn, approx 15 cm from turn signal flasher | 8A-201-29 Fig 54 | -- | --
S214 | Body harn, approx 16.5 cm from turn signal flasher | 8A-201-29 Fig 54 | -- | --
S225 | Body harn, approx 8 cm from G201 | 8A-201-31 Fig 59 | -- | --
S245 | Body harn, approx 38 cm from PCM conn | 8A-201-29 Fig 54 | -- | --
S248 | Body harn, approx 43.5 cm from PCM conn | 8A-201-29 Fig 54 | -- | --
S258 | Body harn, approx 18 cm from turn signal flasher | 8A-201-29 Fig 54 | -- | --
S259 | Body harn, approx 102.5 cm from PCM conn | 8A-201-29 Fig 54 | -- | --
S261 | Body harn, approx 19.5 cm from PCM conn | 8A-201-29 Fig 54 | -- | --
S282 | Body harn, approx 55 cm from PCM conn | 8A-201-29 Fig 54 | -- | --
S290 | Body harn, approx 29 cm from P500 | 8A-201-22 Fig 42 | -- | --
S295 | Body harn, approx 3 cm from PCM conn | 8A-201-31 Fig 59 | -- | --
S297 | Body harn, approx 34 cm from PCM conn | 8A-201-29 Fig 54 | -- | --
S298 | Body harn, approx 38.5 cm from P500 | 8A-201-22 Fig 42 | -- | --
S334 | Body harn, approx 1.5 cm from P402 | 8A-201-38 Fig 72 | -- | --
S361 | Body harn, approx 10.5 cm from P402 | 8A-201-42 Fig 81 | -- | --
S365 | Body harn, approx 26 cm into cross car breakout | 8A-201-42 Fig 81 | -- | --
S427 | Body harn, approx 13 cm from C303 | 8A-201-42 Fig 81 | -- | --