For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Data Link Connector (DLC) | Under the left side of the IP, to the left of the steering column | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
IP Fuse Block | On the left front side of the passenger compartment, attached to the door hinge pillar | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Powertrain Control Module (PCM) (Buick) | Under the right side of the IP, near the rear of the IP compartment | Engine Controls Component Views in Engine Controls - 3.8L | Engine Controls Connector End Views in Engine Controls - 3.8L
Powertrain Control Module (PCM) (Oldsmobile) | Under the right side of the IP, near the rear of the IP compartment | Engine Controls Component Views in Engine Controls - 4.0L | Engine Controls Connector End Views in Engine Controls - 4.0L
Variable Steering Actuator | On the right rear side of the engine compartment, on the power steering rack | Steering Assist Component Views | Steering Assist Connector End Views
Variable Steering Module | Under the right side of the IP, on the left side of the HVAC case | Steering Assist Component Views | Steering Assist Connector End Views
C101 (78 cavities) (VIN 1) | Body harness to the transmission harness, on the center rear of the engine compartment | Harness Routing Views in Wiring Systems | --
C101 (78 cavities) (VIN C) | Body harness to the transmission harness, on the center rear of the engine compartment | Harness Routing Views in Wiring Systems | --
G202 | On the left front side of the passenger compartment, under the kick panel trim plate | Harness Routing Views in Wiring Systems | --
P100 | On the left rear side of the engine compartment, near the base of the strut tower | Harness Routing Views in Wiring Systems | --
P107 | On the right rear side of the engine compartment, near the base of the strut tower | Harness Routing Views in Wiring Systems | --
S209 | In the body harness, approximately 37.5 cm (14.7 in) from the turn signal flasher | Harness Routing Views in Wiring Systems | --
S214 | In the body harness, approximately 39 cm (15.3 in) from the turn signal flasher | Harness Routing Views in Wiring Systems | --
S259 | In the body harness, approximately 160.5 cm (63.2 in) from the PCM | Harness Routing Views in Wiring Systems | --
S290 | In the body harness, approximately 73 cm (28.7 in) from P100 | Harness Routing Views in Wiring Systems | --
S298 | In the body harness, approximately 82.5 cm (32.4 in) from P100 | Harness Routing Views in Wiring Systems | --
S365 | In the body harness, approximately 132 cm (51.9 in) from P800 | Harness Routing Views in Wiring Systems | --
S410 | In the body harness, approximately 37 cm (14.5 in) from G401 | Harness Routing Views in Wiring Systems | --