For 1990-2009 cars

# SUNROOF CABLE REPLACEMENT REPLACE CABLES IN PAIRS

WHEN A RIGHT OR LEFT SUNROOF DRIVE CABLE ASSEMBLY IS DAMAGED, BOTH ASSEMBLIES MUST BE REPLACED. THIS IS DONE TO ASSURE EVEN PARALLEL TRAVEL OF THE SUNROOF ASSEMBLY. LEFT AND RIGHT CABLE ASSEMBLIES ARE PART OF A SERVICE KIT: PART NUMBERS: 20495001 - MODELS A,E,G & K PART NUMBERS: 20495002 - - B & C AVAILABLE FROM GENERAL MOTORS PARTS DEPARTMENT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.