For 1990-2009 cars

## Instrument Cluster Lens Replacement Buick

### Removal Procedure

1. Remove the instrument cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the lens screws from the instrument cluster (2).
3. Remove the lens.

### Installation Procedure

1. Install the lens to the instrument cluster (2).
2. Install the lens screws to the instrument cluster (2).
3. Install the instrument cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .

## Instrument Cluster Lens Replacement Oldsmobile

### Removal Procedure

1. Remove the instrument cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the lens screws to the instrument cluster (2).
3. Remove the lens.

### Installation Procedure

1. Install the instrument cluster lens to the instrument cluster (2).
2. Install the lens screws to the instrument cluster (2).
3. Install the trim plate. Refer to Instrument Cluster Trim Panel Replacement .