For 1990-2009 cars

Table 1: | Radio (Buick)
Table 2: | Radio (Oldsmobile)
Table 3: | Audio Amplifier (Bose®)
Table 4: | Compact Disc (CD) Player
Table 5: | Left Front Door Speaker
Table 6: | Left Front Door Speaker (Tweeter)
Table 7: | Left Rear Door Speaker (w/UIF)
Table 8: | Power Antenna Relay
Table 9: | Right Front Door Speaker
Table 10: | Right Front Door Speaker (w/UF1)
Table 11: | Right Rear Door Speaker (w/UF1)

#### Radio (Buick)

Connector Part Information |

• | 12110115

• | 32-Way F Micro-Pack 100 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
E1 | DK GRN | 835 | Diagnostic Signal E & C
E2-E3 | -- | -- | Not Used
E4 | PPL/WHT | 724 | Vacuum Fluorescent Dimming Signal
E5 | LT GRN | 1011 | Remote Radio Control Signal
E6-E8 | -- | -- | Not Used
E9 | BLK/WHT | 372 | Remote Radio Return - Audio
E10 | BRN/WHT | 367 | Remote Radio Signal - Left Audio
E11 | DK GRN/ WHT | 368 | Remote Radio Signal - Right Audio
E12 | BRN | 199 | Speaker Feed Left Rear
E13 | YEL | 116 | Speaker Return Left Rear
E14 | DK GRN | 117 | Speaker Return - Right Front
E15 | LT GRN | 200 | Speaker Feed- Right Front
E16 | BLK/WHT | 351 | Ground
F1 | ORN | 440 | Fused Output - BAT
F2 | YEL | 43 | Fuse Output - Accessory
F3 | DK GRN | 145 | Power Antenna Relay Feed Coil
F4 | GRY | 8 | IP Lamp Feed
F5 | YEL | 390 | Instrument Panel Lamp Feed
F6-F7 | -- | -- | Not Used
F8 | BLK/WHT | 351 | Ground
F9 | BLK/WHT | 351 | Ground
F10 | BLK/WHT | 351 | Ground
F11 | BARE | 1782 | Drain Wire Return
F12 | TAN | 201 | Speaker Feed Left Front
F13 | GRY | 118 | Speaker Return Left Front
F14 | LT BLU | 115 | Speaker Return Right Rear
F15 | DK BLU | 46 | Speaker Feed Right Rear
F16 | -- | -- | Not Used

#### Radio (Oldsmobile)

Connector Part Information |

• | 12110115

• | 32-Way F Micro-Pack 100 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
E1 | DK GRN | 835 | Diagnostic Signal E & C
E2 | -- | -- | Not Used
E3¹ | PNK | 608 | Reference Voltage Feed -- 14-Volt Reference
E4 | -- | -- | Not Used
E5 | LT GRN | 1011 | Remote Radio Control Signal
E6-E8 | -- | -- | Not Used
E9² | BLK/WHT | 372 | Remote Radio Return - Audio
E10² | BRN/WHT | 367 | Remote Radio Signal - Left Audio
E11² | DK GRN/ WHT | 368 | Remote Radio Signal - Right Audio
E12 | BRN | 199 | Speaker Feed -- Left Rear
E12¹ | BRN | 599 | Audio Signal -- Left Rear Low Level
E13³ | YEL | 116 | Speaker Return -- Left Rear
E14³ | DK GRN | 117 | Speaker Return -- Right Front
E15 | LT GRN | 200 | Speaker Feed -- Right Front
E15¹ | DK BLU | 546 | Audio Signal -- Right Rear Low Level
E16 | BLK/WHT | 351 | Ground
F1 | ORN | 440 | Fused Output - BAT
F2 | YEL | 43 | Fuse Output - Accessory
F3 | DK GRN | 145 | Power Antenna Relay Feed Coil
F4 | BRN | 1244 | Instrument Panel Lamp Feed #2
F5 | YEL | 390 | Instrument Panel Lamp Feed
F6-F11 | -- | -- | Not Used
F12 | TAN | 201 | Speaker Feed -- Left Front
F12¹ | TAN | 511 | Audio Signal Left Front Low Level
F13 | GRY | 118 | Speaker Return Left Front
F13¹ | BARE | 1782 | Drain Wire Return
F14 | LT BLU | 115 | Speaker Return Right Rear
F14¹ | WHT | 513 | Speaker Return Low Level
F15 | DK BLU | 46 | Speaker Feed Right Rear
F15¹ | LT GRN | 512 | Audio Signal- Right Front Low Level
F16 | -- | -- | Not Used
¹ Bose® System (UU8)
² With CD Changer (U1S)
³ Base Radio (UL0)

#### Audio Amplifier (Bose®)

Connector Part Information |

• | 12110088

• | 24-Way F Metri-Pak

• | 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | PNK | 608 | Reference Voltage Feed - 14 Volt Reference
A2 | RED | 1242 | Fuse Output -Battery
A3 | RED | 1242 | Fuse Output - Battery
A4 | RED | 1242 | Fuse Output - Battery
A5 | YEL | 116 | Speaker Return - Left Rear
A6 | DK GRN | 117 | Speaker Return - Right Front
A7 | LT GRN | 200 | Speaker Feed - Right Front
A8 | BRN | 199 | Speaker Feed - Left Rear
A9 | TAN | 201 | Speaker Feed - Left Front
A10 | GRA | 118 | Speaker Return - Left Front
A11 | DK BLU | 46 | Speaker Feed - Right Rear
A12 | LT BLU | 115 | Speaker Return - Right Rear
B1 | -- | -- | Not Used
B2 | BLK/WHT | 251 | Ground - Clean
B3 | BLK/WHT | 251 | Ground - Clean
B4 | BLK/WHT | 251 | Ground - Clean
B5-B7 | -- | -- | Not Used
B8 | WHT | 513 | Speaker Return - Low Level
B9 | LT GRN/BLK | 512 | Audio Signal - Right Front - Low Level
B10 | BRN | 599 | Audio Signal - Left Rear - Low Level
B11 | DK BLU | 546 | Audio Signal - Right Rear - Low Level
B12 | TAN | 511 | Audio Signal - Left Front - Low Level

#### Compact Disc (CD) Player

Connector Part Information |

• | 12047531

• | 10-Way F Metri-Pak

• | 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/WHT | 367 | Remote Radio Signal - Left Audio
2 | DK GRN/ WHT | 368 | Remote Radio Signal - Right Radio
3 | BLK/WHT | 372 | Remote Radio Return - Audio
4 | BARE | 514 | Drain Wire Return
5 | ORN | 440 | Fuse Output - Battery
6 | -- | -- | Not Used
7 | BLK | 1051 | Radio Ground
8-9 | -- | -- | Not Used
10 | DK GRN | 835 | Diagnostic Signal - Entertainment and Comfort

#### Left Front Door Speaker

Connector Part Information |

• | 12052832

• | 2-Way F Metri-Pak

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 118 | Speaker Return - Left Front
B | TAN | 201 | Speaker Feed - Left Front

#### Left Front Door Speaker (Tweeter)

Connector Part Information |

• | 12064750

• | 2-Way M Metri-Pak

• | 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 118 | Speaker Return - Left Front
B | TAN | 201 | Speaker Feed - Left Front

#### Left Rear Door Speaker (w/UIF)

Connector Part Information |

• | 12052832

• | 2-Way F Metri-Pak

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 116 | Speaker Return - Left Rear
B | BRN | 199 | Speaker Feed - Left Rear

#### Power Antenna Relay

Connector Part Information |

• | 12010013

• | 3-Way F Metri-Pak

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 440 | Fuse Output - Battery
B | DK GRN | 145 | Power Antenna Relay Feed - Coil
C | BLK | 1050 | Ground

#### Right Front Door Speaker

Connector Part Information |

• | 12052832

• | 2-Way F Metri-Pak

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 117 | Speaker Return - Right Front
B | LT GRN | 200 | Speaker Feed - Right Front

#### Right Front Door Speaker (w/UF1)

Connector Part Information |

• | 12064750

• | 2-Way M Metri-Pak

• | 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 117 | Speaker Return - Right Front
B | LT GRN | 200 | Speaker Feed - Right Front

#### Right Rear Door Speaker (w/UF1)

Connector Part Information |

• | 12052832

• | 2-Way F Metri-Pak

• | 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 115 | Speaker Return - Right Rear
B | DK BLU | 46 | Speaker Feed - Right Rear