For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Diagonal Braces to Radiator Opening | 10.5 N·m | 93 lb in
Engine Compartment Rear Brace | 50 N·m | 37 lb ft
Fender at Headlamp Opening | 10.5 N·m | 93 lb in
Fender to Door Hinge Pillar | 9 N·m | 80 lb in
Fender to Upper Rail | 9 N·m | 80 lb in
Front End Lower Brace | 50 N·m | 37 lb ft
Front End Panel | 10.5 N·m | 93 lb in
Front End Upper Brace | 22 N·m | 16 lb ft
Grille to Hood | 1.9 N·m | 17 lb ft
Hood Hinge Pivot Bolts | 10.5 N·m | 93 lb in
Hood Hinge to Body | 10.5 N·m | 93 lb in
Hood Hinge to Hood | 10.5 N·m | 93 lb in
Hood Latch Support | 10.5 N·m | 93 lb in
Hood Latch to Latch Support | 18 N·m | 13 lb ft
Latch Striker to Hood | 10.5 N·m | 93 lb in
Upper Radiator Support | 10.5 N·m | 93 lb in
Wheel Nuts | 140 N·m | 100 lb ft