For 1990-2009 cars

# REVISED CYLINDER HEAD BOLT TORQUING PROCEDURE

#### MODELS AFFECTED: 1989-90 ELECTRA WITH 3800 (VIN CODE C) 1989-90 LESABRE WITH 3800 (VIN CODE C) 1989-90 RIVIERA/REATTA WITH 3800 (VIN CODE C)

#### IMPORTANT: This bulletin revises the cylinder head bolt torquing procedure for 3800 (VIN C) that appears in the 1989 and 1990 Service Manuals. The procedure for the 3800 (VIN C) is the same as that for the 3300 (VIN N). The bolt torquing sequence remains the same for both engines.

INSTALL OR CONNECT

1. Clean threads in the block using a 7/16-14 tap

2. Clean bolt threads using a wire brush

3. Cylinder head gasket on block

4. Apply sealant, GM part number 1052080, on bolt threads

5. Cylinder head bolts

6. Tighten cylinder head bolts to 47 N.m (35 lbs.ft.) in sequence

7. Rotate each bolt 130 DEG in sequence using J36660 Torque, Angle Meter.

8. Rotate the center four bolts an additional 30 DEG in sequence using J36660, Torque Angle Meter.

9. Pushrods, guide plate and rocker arm assemblies

Apply threadlock, GM part number 12345493, to rocker arm pedestal bolts before assembly

Tighten rocker arm pedestal bolts to 38 N.m (28 lbs. ft.)

10. Intake manifold

11. Valve cover

12. Exhaust manifold:

Front (left) cylinder head

A/C compressor bracket bolt to 70 N.m (52 lbs. ft.) Generator support bracket to cylinder head Generator C3I and spark plug wires Rear (right) cylinder head Belt tensioner assembly Power steering pump Fuel line heat shield

13. Negative battery cable

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.