For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pipe Primary and Secondary Connections at the Master Cylinder | 17 N·m | 13 lb ft
Brake Pipes to BPMV | 15 N·m | 11 lb ft
BPMV Bracket to Side Rail Bolts | 27 N·m | 20 lb ft
BPMV Bracket to Side Rail Bracket Bolts | 27 N·m | 20 lb ft
BPMV Mounting Bracket Bolt | 8 N·m | 71 lb in
BPMV Mounting Bracket Nut | 20 N·m | 15 lb ft
Proportioner Valves to Brake Pipe Fittings | 15 N·m | 11 lb ft
Rear Wheel Speed Sensor Screws | 3.7 N·m | 33 lb in
Side Rail Bracket Bolts | 26 N·m | 19 lb ft
Valve Block to Pump and Motor Assembly Bolts | 19 N·m | 21.4 lb ft