For 1990-2009 cars

## Front Air Deflector Replacement Oldsmobile

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the push-in retainers (2) retaining the lower air deflector (1).
3. Remove the lower air deflector (1).

### Installation Procedure

1. Install the lower air deflector (1).
2. Install the push-in retainers (2).
3. Lower the vehicle.

## Front Air Deflector Replacement Buick

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the push-in retainers (2) that retain the lower air deflector (1).
3. Remove the lower air deflector (1).

### Installation Procedure

1. Install the lower air deflector (1).
2. Install the push-in retainers (2).
3. Lower the vehicle.