For 1990-2009 cars

## Rear Compartment Side Trim Replacement - Right Side Oldsmobile

### Removal Procedure

1. Remove the cargo net from the retainers.
2. Remove the push-in retainers (5).
3. Remove the cargo net retainers (6).
4. Remove the rear compartment side trim (3) from the vehicle.

### Installation Procedure

1. Install the rear compartment side trim (3) to the vehicle.
2. Install the push-in retainers (5).
3. Install the cargo net retainers (6).
4. Install the cargo net to the retainers.

## Rear Compartment Side Trim Replacement - Right Side Buick

### Removal Procedure

1. Remove the cargo net from the retainers.
2. Remove the push-in retainers (3).
3. Remove the cargo net retainers (2).
4. Remove the rear compartment side trim (1) from the vehicle.

### Installation Procedure

1. Install the rear compartment side trim (1) to the vehicle.
2. Install the push-in retainers (3).
3. Install the cargo net retainers (2).
4. Install the cargo net to the retainers.