For 1990-2009 cars

### Removal Procedure

1. Remove the trim panel (3). Refer to Front Side Door Trim Panel Replacement or Rear Side Door Trim Panel Replacement .
2. Remove the trim panel plate (1). Refer to Door Trim Plate Replacement .
3. Remove the screws that retain the power window switch.
4. Remove the power window switch assembly (1).

### Installation Procedure

1. Install the power window switch assembly .
2. Install the screws in order to retain the power window switch.
3. Install the trim panel plate (1). Refer to Door Trim Plate Replacement .
4. Install the trim panel (3). Refer to Front Side Door Trim Panel Replacement or Rear Side Door Trim Panel Replacement .