For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Instrument Cluster
2 | Inspect the following connectors for proper connections:

• | Instrument cluster connector C1

• | Instrument cluster connector C2

Are the connections OK?

--

Go to Step 4

Go to Step 3

3 | Repair the poor connection. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
4 | Replace the instrument cluster. Refer to Instrument Cluster Replacement . Is the replacement complete? | -- | Go to Instrument Cluster System Check | --