For 1990-2009 cars

## Instrument Panel Center Trim Panel Replacement Buick

### Removal Procedure

1. Remove the pin retainers (2) by pushing in the retainer buttons.
2. Remove the upper trim plate (1) from the instrument panel trim pad.

### Installation Procedure

1. Install the upper trim plate (1) to the instrument trim pad.
2. Reset the retainers by returning each button to the outward position.
3. Install the retainers (2).
4. Snap the retainer pins flush with the retainer head.

## Instrument Panel Center Trim Panel Replacement Oldsmobile

### Removal Procedure

1. Pull the trim plate (1) rearward in order to release the retainers.
2. Remove the trim plate (1).

### Installation Procedure

1. Align the trim plate retainers and the locating pins to the instrument panel assembly.
2. Push inward in order to fasten the trim plate (1).