For 1990-2009 cars

## Rear Seat Back Cushion Cover Replacement Buick

### Removal Procedure

1. Remove the seat cushion assembly. Refer to Rear Seat Cushion Replacement .
2. Remove the seat back assembly. Refer to Rear Seat Back Replacement .
3. Remove the hog rings on the perimeter of the seat back cushion (2).
4. Remove the seat back cover (3) from the seat back cushion (2).

### Installation Procedure

1. Install the seat back cover (3) in position on the seat back cushion (2).
2. Install the hog rings on the perimeter of the seat back cushion (2).
3. Install the seat back assembly. Refer to Rear Seat Back Replacement .
4. Install the seat cushion assembly. Refer to Rear Seat Cushion Replacement .

## Rear Seat Back Cushion Cover Replacement Oldsmobile

### Removal Procedure

1. Remove the seat cushion assembly. Refer to Rear Seat Cushion Replacement .
2. Remove the seat back assembly. Refer to Rear Seat Back Replacement .
3. Remove the hog rings on the perimeter of the seat back cover (1).
4. Remove the seat back cover (1) from the seat back cushion.

### Installation Procedure

1. Install the seat back cover (1) in position on the seat back cushion.
2. Install the hog rings on the perimeter of the seat back cushion (1).
3. Install the seat back assembly. Refer to Rear Seat Back Replacement .
4. Install the seat cushion assembly. Refer to Rear Seat Cushion Replacement .