For 1990-2009 cars

# BASECOAT/CLEARCOAT PAINT PLANT PRODUCTION CHANGES

1986 OKLAHOMA CITY PRODUCTION COLOR MATCH

#### MODELS AFFECTED: 1986 CENTURY (VIN PLANT CODE 6) ---------------- Vehicles produced at the Oklahoma City Assembly plant will be painted with the basecoat/clearcoat (BC/CC) system. To achieve an acceptable color match, when paint repairing these vehicles, the new formulation of lacquer/enamel colors must be used (see attached list). To aid in identifying Oklahoma City built vehicles, the eleventh position in the VIN number will be a 6.

Follow the paint manufacturer recommendations when repairing the BC/CC finishes.

PAINT FISHER PPG CODE COLOR WA # DITZLER DUPONT ----- ----- ------ ------- ------ 11 B/C White 3967 3919 D8601

12 B/C Silver * 8535 3920 D8602 15 B/C Med. Gray* 8573 3921 D8603 19 B/C Black 848 9700 99S

25 B/C Lt. Blue* 8574 3922 D8604 31 B/C Dk. Blue* 8592 3923 D8605 43 B/C Lt. Sage* 8572 3924 D8606 54 B/C Yellow Beige 8525 3925 D8607 58 B/C Lt. Chestnut* 8575 3926 D8608 62 B/C Dk. Chestnut* 8593 3927 D8609 71B/C Med. Red* 8772 3928 D8611 79B/C Dk. Red* 8529 3929 D8610

INMONT/ PAINT RINSHED SHERWIN-WILLIAMS MARTIN CODE COLOR MASON (ACME/ROGERS) SENOUR ----- ----- ------- ---------------- ------ 11 B/C White 16456 FA10A2864 82-1871 (5644) 12 B/C Silver * 16445 34380 82-5845 15 B/C Med. Gray* 16446 34381 82-5846 19 B/C Black 403 F10B1738 8800 (4950/4080) 25 B/C Lt. Blue* 16447 37382 82-5847 31 B/C Dk. Blue* 16448 34875 82-5942 43 B/C Lt. Sage* 16449 34386 82-5851 54 B/C Yellow Beige 16450 34861 82-5939 58 B/C Lt. Chestnut* 16451 34396 82-5861 62 B/C Dk. Chestnut* 16452 34398 82-5863 71 B/C Med. Red* 16453 35319 82-6002 79 B/C Dk. Red* 16454 34405 82-5870

B/C - to identify Basecoat/Clearcoat * Metallic

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.