For 1990-2009 cars

### Removal Procedure

1. Remove the outer washer solvent container from the vehicle. Refer to Windshield Washer Solvent Container Replacement .
2. Remove the washer pump from the washer solvent container.

2.1. | Pull the top of the washer pump out from the side of the washer solvent container.

2.2. | Pull the washer pump up out of the washer solvent container.

### Installation Procedure

1. Install the washer pump onto the washer solvent container.

1.1. | Push the washer pump down into the washer solvent container completely.

1.2. | Push the top of the washer pump into the side of the washer solvent container.

2. Install the washer solvent container onto the vehicle. Refer to Windshield Washer Solvent Container Replacement .