For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Bose® Amplifier | In the front of the rear compartment, under the rear package shelf | Entertainment Component Views | --
Compact Disc (CD) Player | In the right side of the rear compartment, near the wheel house | Entertainment Component Views | --
Data Link Connector (DLC) | Under the left side of the IP, to the left of the steering column | Data Link Communications Component Views in Wiring Systems | Data Link Communications Connector End Views in Wiring Systems
Inflatable Restraint Steering Wheel Module Coil | Left front of the passenger compartment, below the steering wheel | SIR Component Views in SIR | --
IP Fuse Block | In the left side of the passenger compartment, attached to the door hinge pillar | Power and Grounding Component Views in Wiring Systems | --
Power Antenna Relay | Right side of the rear compartment, near the wheelhouse | Entertainment Component Views | --
Radio (Buick) | In the center of the IP, near the heater and A/C control | -- | Entertainment Connector End Views
Radio (Oldsmobile) | In the center of the IP, near the heater and A/C control | -- | Entertainment Connector End Views
RH Rear Junction Block | Right rear of the passenger compartment, under the rear seat cushion | Power and Grounding Component Views in Wiring Systems | --
Steering Wheel Control Switches | Left front of the passenger compartment, on the steering wheel | -- | --
C202 (48 cavities) | Body harness to the steering column harness, under the left side of the instrument panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C208 (6 cavities) | Instrument panel, under the left side of the instrument panel | Harness Routing Views in Wiring Systems | --
C209 (4 cavities) | Body harness, under the left side of the instrument panel | Harness Routing Views in Wiring Systems | --
C212 (10 cavities) | Instrument panel harness to the audio harness, under the left side of the instrument panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C215 (8 cavities) | Instrument panel harness to the audio harness, under the left side of the instrument panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C400 (16 cavities) | Instrument panel harness to the audio harness, left rear of the passenger compartment | -- | Inline Harness Connector End Views in Wiring Systems
C501 (10 cavities) (Buick) | Body harness to the door trim harness, in the left front door | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C501 (16 cavities) (Oldsmobile) | Body harness to the door trim harness, in the left front door | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C601 (16 cavities) | Body harness to the door trim harness, in the right front door | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G202 | Left front of the passenger compartment, under the kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
G302 | Left rear of the passenger compartment, under the rear seat cushion | Power and Grounding Component Views in Wiring Systems | --
P500 | Front of the left front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
P600 | Front of the right front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
S209 | In the body harness, approximately 37.5 cm (14.7 in) from the turn signal flasher | Harness Routing Views in Wiring Systems | --
S228 | In the body harness, approximately 20 cm (7.8 in) from the park brake switch | Harness Routing Views in Wiring Systems | --
S231 | In the body harness, approximately 54.5 cm (21.5 in) from the C200 connector | Harness Routing Views in Wiring Systems | --
S232 | In the audio harness, approximately 34.5 cm (13.6 in) from the radio amplifier | Harness Routing Views in Wiring Systems | --
S236 | In the instrument panel harness, approximately 30 cm (12 in) from the C200 connector | Harness Routing Views in Wiring Systems | --
S237 | In the body harness, approximately 24 cm (9.4 in) from the park brake switch | Harness Routing Views in Wiring Systems | --
S246 | In the instrument panel harness, approximately 23.5 cm (9.25 in) from the C200 connector | Harness Routing Views in Wiring Systems | --
S263 | In the body harness, approximately 28 cm (11 in) from the park brake switch | Harness Routing Views in Wiring Systems | --
S264 | In the instrument panel harness, approximately 56.5 cm (22.2 in) from the radio | Harness Routing Views in Wiring Systems | --
S290 | In the body harness, approximately 73 cm (29 in) from the P100 pass-through | Harness Routing Views in Wiring Systems | --
S298 | In the body harness, approximately 82.5 cm (32.5 in) from the P100 pass-through | Harness Routing Views in Wiring Systems | --
S366 | In the body harness, approximately 111 cm (43.7 in) from the P800 pass-through | Harness Routing Views in Wiring Systems | --
S418 | In the body harness, approximately 92 cm (36 in) from the P800 pass-through | Harness Routing Views in Wiring Systems | --
S451 | In the body harness, approximately 150 cm (59.1 in) from the P800 pass-through | -- | --