For 1990-2009 cars

# NEW WIRING HARNESS AND PRESSURE SWITCHES

#### MODELS AFFECTED: 1990 CENTURY, LESABRE, PARK AVENUE, RIVIERA, REATTA AND REGAL EQUIPPED WITH THM 440T4/HYDRA-MATIC 4T60

BULLETIN COVERS: (Figures 1, 2, 3 and 4)

The 2nd, 3rd and 4th clutch circuit pressure switches will have "button-headed" wire connectors instead of blade type connectors for easier assembly at the transaxle assembly plant and to reduce the chance of the connectors working loose. This change also requires new wiring harnesses.

#### SERVICE PROCEDURE

The new pressure switches and wiring harnesses will be available for service.

#### DATE OF PRODUCTION CHANGE

Starting September 6, 1989 (Julian Date 249), some Hydra-Matic 4T60 (THM 440-T4) transaxles were built using the new pressure switches and wiring harnesses. Since early November, 1989, all models have the new pressure switches and wiring harnesses.

#### SERVICE PARTS INFORMATION

Listed below are the service part numbers for the new pressure switches and wiring harnesses.

Model Part Number Description Year Model Usage ----------- ----------- ---- ------------

12096136 Harness Assembly, Wiring 1990 BHH, BJH, BPH, BWH, YKH, LAH, LMH, LNH, PAH

12096137 Harness Assembly, Wiring 1990 BAH, BDH, BFH, BMH, CDH

12096127 Harness Assembly, Wiring 1990 AAH, ABH, AFH, AJH ANH, ATH

12096322 Harness Assembly, Wiring 1990 AXH (THM F-7)

8668271 Clip, Wire Conduit (TCC/VCC) 1990 All

8668707 Switch Assembly - Pressure 1990 AAH, ABH, AFH, AJH, (4th Clutch) (N.C.) ANH, ATH, BAH, BDH, BFH, BHH, CDH, CLH, CPH, CYH, CZH, BJH, BPH, BWH, CHH, LAH, LCH, LMH, LNH, PAH

8668707 Switch Assembly - Pressure 1990 AAH, ABH, AFH, AJH, (3rd Clutch) (N.C.) ANH, ATH, BAH, BDH, BFH, BHH, CDH, CLH, CPH, CYH, CZH, BJH, BPH, BWH, CHH, LAH, LCH, LMH, LNH, PAH

8668707 Switch Assembly - Pressure 1990 BHH, BJH, BPH, BWH, (2nd Clutch) (N.C.) CHH, CJH, LAH, LCH, LMH, LNH, PAH

Parts are expected to be available on 12-15-89. Until then normal part orders will not be accepted by GMSPO. Only verifiable emergency VIP orders will be accepted. SPO will make every effort to obtain parts. All parts will be placed on 400 control to waive VIP surcharges. However, the part will be shipped premium transportation at dealer's expense. All other order types will be canceled as incorrectly ordered while the 400 control is in place.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.