Vibration or Rattling. Buick Roadmaster 1996

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check to see if the exhaust component is contacting the body component. Is the exhaust component contacting the body component? | -- | Go to Step 2 | Go to Step 3

2

1. Loosen the clamps.
2. Realign the exhaust system.

Is the exhaust system vibrating?

--

Go to Step 3

System OK

3 | Check to see if the exhaust vibration dampener is loose, damaged or missing. Is the exhaust vibration dampener loose, damaged or missing? | -- | Go to Step 4 | Go to Step 5
4 | Tighten or replace the exhaust vibration dampener. Is the exhaust system vibrating? | -- | Go to Step 5 | System OK
5 | Check to see if the exhaust pipes are contacting the heat shields. Are the exhaust pipes contacting the heat shields? | -- | Go to Step 6 | --

6

1. Loosen the clamps.
2. Realign the exhaust system.

Is the exhaust system vibrating?

--

--

System OK