SERVICE MANUAL UPDATE SEC. 8A KEYLESS PROGRAMMING CONNECTOR. Buick Roadmaster 1992

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 8A KEYLESS PROGRAMMING CONNECTOR

#### SUBJECT: SMU - SECTION 8A, 9K - REVISED KEYLESS PROGRAMMING CONNECTOR LOCATION

#### VEHICLES AFFECTED: 1992 "B" MODELS WAGONS CHEVROLET CAPRICE WAGON OLDSMOBILE CUSTOM CRUISER WAGON BUICK ROADMASTER WAGON

SERVICE MANUAL UPDATE SECTION 8A, 9K

- - - - - - - - - - -

This bulletin serves to update Service Manual Keyless Entry Connector Locations.

The Keyless Entry Programming Connector on the 1992 "B" Wagons can be found under the left quarter trim panel.

This description will replace the Keyless Entry Programming Connector Component Location found on the following pages:

CHEVROLET - 8A 132-1 BUICK - 8A 132-3 OLDSMOBILE - 8A 132-2

For removal and reinstallment procedures of the left quarter trim panel refer to "Rear Quarters" in Section 10-7 of the 1992 Service Manual.

Refer to the attached diagram for a component location view. The attached diagram will replace diagrams on the following pages:

BUICK - 9K-4, Figure 5 OLDSMOBILE - 9K-2, Figure 3

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.