INFO. ON FRONT OR REAR WINDOW INOP. CAUSED BY DETACHMENT OF. Buick Roadmaster 1992

For 1990-2009 cars

# INFO. ON FRONT OR REAR WINDOW INOP. CAUSED BY DETACHMENT OF

THIS IS A MONTHLY SERVICE NEWSLETTER ARTICLE. THIS BULLETIN IS NOT INTENDED FOR PUBLICATION.

#### SUBJECT: INFORMATION ON FRONT OR REAR WINDOW INOPERATIVE CAUSED BY DETACHMENT OF LOWER SASH

#### MODELS: 1991-96 BUICK ROADMASTER

THE FRONT OR REAR OF THE LOWER WINDOW SASH MAY DETACH FROM THE WINDOW REGULATOR ASSEMBLY. PART NUMBER 20369894 (CLIP) WILL REPLACE THE MISSING CLIP. THE CLIP IS LISTED IN THE PARTS BOOK AS AN H CAR CLIP BUT WILL FIT THE B CAR. THE END OF THE REGULATOR IS STAKED AND THIS STAKE MUST BE REMOVED PRIOR TO USING A PAIR OF PLIERS TO INSTALL THE CLIP.

#### PARTS INFORMATION:

PARTS ARE CURRENTLY AVAILABLE THROUGH GMSPO.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.