Automatic Transmission Components. Buick Roadmaster 1996

For 1990-2009 cars

#### B car CompLoc

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
1-2 Shift Solenoid Valve (1-2 SS Valve ) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission Automatic Transmission Inline Harness Connector End View | --
2-3 Shift Solenoid Valve (2-3 SS Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission Automatic Transmission Inline Harness Connector End View | --
3-2 Shift Solenoid Valve Assembly | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission Automatic Transmission Inline Harness Connector End View | --
Automatic Transmission Fluid Pressure Manual Valve Position Switch (TFP Val. Position Sw.) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission Automatic Transmission Inline Harness Connector End View | --
Automatic Transmission Fluid Temperature Sensor (TFT Sensor) | In the TFP Val. Position Sw. | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission Automatic Transmission Inline Harness Connector End View | --
Cruise Control Release Switch | Below LH side of IP, mounted on the brake pedal support | -- | -- | --
IP Fuse Block | Mounted to LH IP, accessible with the LH front door open | 8A-201-11 Fig 19 | 8A-11-0 | --
Powertrain Control Module (PCM) | Engine compartment, forward of LH wheelhouse under the air cleaner | 6 - Engine Controls | -- | --
C1 (32 cavities) | Engine harness to PCM, engine compartment, forward of LH wheelhouse, under the air cleaner | -- | 6 - Engine Controls | --
C2 (32 cavities) | Engine harness to PCM, engine compartment, forward of LH wheelhouse, under the air cleaner | -- | 6 - Engine Controls | --
C3 (32 cavities) | Engine harness to PCM, engine compartment, forward of LH wheelhouse, under the air cleaner | -- | 6 - Engine Controls | --
C4 (32 cavities) | Engine harness to PCM, engine compartment, forward of LH wheelhouse, under the air cleaner | -- | 6 - Engine Controls | --
Pressure Control Solenoid Valve (PC SOL. Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission Automatic Transmission Inline Harness Connector End View | --
Torque Converter Clutch Pulse Width Modulation Solenoid Valve (TCC PWM Sol. Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission Automatic Transmission Inline Harness Connector End View | --
Torque Converter Clutch Solenoid Valve (TCC Sol. Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission Automatic Transmission Inline Harness Connector End View | --
Torque Converter Clutch (TCC) Temperature Switch | In the transmission cooler pipe, near the cooler | 7 - Automatic Transmission | 7 - Automatic Transmission | --
Underhood Electrical Center | Engine compartment, attached to the RH wheelhouse | 8A-201-6 Fig 13 | 8A-11-3 | --
Vehicle Speed Sensor (VSS) | Rear RH side of the transmission | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
C204 (37 cavities) | Body to engine harness, behind RH side of IP, between the blower motor and IP compartment | 8A-201-17 Fig 28 | 8A-202-3 | --
P100 | RH IP, forward of the blower motor | 8A-201-6 Fig 13 | -- | --
S114 | Engine harness, about 14 cm from the underhood lamp branch breakout | -- | -- | --
S116 | Engine harness, LH side of the engine compartment about 17 cm form the ground G104 breakout | -- | -- | --
S122 | Engine harness, LH side of the engine compartment about 17 cm from the ground G104 breakout | -- | -- | --
S132 | Engine harness, about 13 cm from the underhood electrical center | -- | -- | --
S230 | Body harness, about 4 cm from the BTSI solenoid connector breakout | -- | -- | --