Fastener Tightening Specifications. Buick Roadmaster 1996

For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Catalytic Converter Nut | 50 | 37 | --
Catalytic Converter Support Bolt | 34 | 25 | --
Catalytic Converter Support Clamp Nut | 35 | 26 | --
Catalytic Converter Heat Shield Bolt | 1.9 | -- | 17
Exhaust Muffler Bolt | 20 | 15 | --
Exhaust Muffler Clamp Nut | 35 | 26 | --
Exhaust Muffler Heat Shield Bolt | 1.9 | -- | 17
Exhaust Muffler Vibration Dampener | 41 | 30 | --
Exhaust Pipe Front Heat Shield Bolt | 1.9 | -- | 17
Exhaust Resonator Rear Hanger Bolt | 17 | 13 | --
Exhaust Tailpipe Front Hanger Bracket Bolt | 50 | 37 | --
Fuel Tank Front Shield Bolt | 1.9 | -- | 17
Fuel Tank Shield Bolt (Sedan) | 1.9 | -- | 17
Fuel Tank Shield Bolt (Wagon) | 6 | -- | 53
Fuel Tank Shield Bracket Bolt | 1.9 | -- | 17