SMU - SECTION 9K - REMOTE KEYLESS ENTRY. Buick Roadmaster 1994

For 1990-2009 cars

# SMU - SECTION 9K - REMOTE KEYLESS ENTRY

---------------------------------------------------------------------- SERVICE MANUAL UPDATE ----------------------------------------------------------------------

#### SUBJECT: SECTION 9K - REMOTE KEYLESS ENTRY

#### MODELS: 1994-95 BUICK ROADMASTER WAGON

THE CORRECT LOCATION FOR THE REMOTE KEYLESS ENTRY SYSTEM PROGRAMMING CONNECTOR IS BEHIND THE LEFT BACK BODY PILLAR FINISH PANEL (LEFT "D" PILLAR). THE SERVICE MANUAL INCORRECTLY STATES THE RIGHT SIDE.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.