INOPERATIVE LOW COOL LIGHT LIGHT OPERATION OUTLINED. Buick Skyhawk 1987

For 1990-2009 cars

# INOPERATIVE LOW COOL LIGHT LIGHT OPERATION OUTLINED

#### MODELS AFFECTED: 1987 SKYHAWKS WITH THE 2.0L OHV L-4 ENGINE (VIN CODE 1)

During the 1987 model year, a change has been made to the low engine coolant light system of 2.0L L-4 (VIN Code 1) Skyhawks. This feature has been cancelled and will no longer be available on these vehicles after VIN HK436904.

This bulletin is for information purposes only.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.