TIMING BELT ADJUSTMENT UPDATED SERVICE PROCEDURE. Buick Skyhawk 1986

For 1990-2009 cars

# TIMING BELT ADJUSTMENT UPDATED SERVICE PROCEDURE

TIMING BELT ADJUSTMENT

#### MODELS AFFECTED: 1982-1986 1.8L OHC ENGINE --------------- (VIN CODE 0 & VIN CODE J)

#### NOTICE: ALL BELT TENSION ADJUSTMENTS ARE TO BE MADE ON A COLD ENGINE. THIS IS A PROCEDURAL CHANGE FROM PREVIOUS BULLETINS AND SECTION 6A1-12, STEP 5, OF THE 1986 SERVICE MANUAL. ALSO PLEASE DISCARD ALL PREVIOUS 1.8L OHC ENGINE TIMING BELT ADJUSTMENT PROCEDURE INSTRUCTIONS.

A new 20mm wide timing belt, Part No. 90234902 has been released for production and service on 1982 thru 1986 1.8L OHC engines.

After a new timing belt is installed and tensioned, the engine must be turned over (without starting) approximately 10 revolutions. As the new belt takes a set position, a substantial tension loss will occur, and the timing belt must then be re-tensioned.

When a new 20mm wide timing belt is installed or an existing 19m wide timing belt is re-tensioned, it must be tensioned to within the band (between the two arrows on perimeter of gage dial face identified as 1.8L OHC) as shown in illustration. The band represents 15ON (30 lbs.) on a cold engine. The timing belt tension gage, J-26486-A was an essential tool which dealers received approximately May, 1982. This same tool was reworked and released for the 1.8L OHC engine. Because of the importance of correct timing belt tensioning, it is imperative all dealerships use the gage that has accurate calibrations.

Use applicable labor time and labor operations for this operation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.