CATALYTIC CONVERTER EXHAUST ODOR-NEW P/N AVAILABLE. Buick Skyhawk 1987

For 1990-2009 cars

# CATALYTIC CONVERTER EXHAUST ODOR-NEW P/N AVAILABLE

#### MODELS AFFECTED: 1987 SKYHAWKS (BELOW VIN HK440902) WITH THE LL8 2.OL L-4 ENGINE (VIN CODE 1) 1987 CENTURYS WITH THE LB6 2.8L V-6 ENGINE (VIN CODE W)

Some of the affected models may exhibit a higher than normal catalytic converter odor during vehicle operation. This odor condition can be reduced by installing a service catalytic converter as specified below:

Carline Engine (VIN Code) Converter ------- ----------------- --------- Century V-6, 2.8L (W) 25104019 Skyhawk L-4, 2.OL (1) 25103456

Use applicable Labor Operation Numbers and Labor Time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.