FRONT SUSPENSION SQUAWKING NOISE- STABILIZER BAR. Buick Skyhawk 1984

For 1990-2009 cars

# FRONT SUSPENSION SQUAWKING NOISE- STABILIZER BAR

VEHCLES AFFECTED: 1984 'J' Series Vehicles

Some early 1984 'J' Series may exhibit a 'squawking' noise which may be caused by the front stabilizer bar bushing when they are subjected to significant jounce/rebound suspension motions. Vehicles experiencing the 'squawking' noise can be repaired by installing two (2) new insulators from the following part number list:

Old P/N New P/N Stabilizer Bar Dia ------- ------- ------------------ 14076617 14085145 24mm (0.945 in.) 14076619 14685147 28mm (1.102 in.) 14076620 14085148 30mm (1.181 in.)

Refer to the illustration for installation procedures and torques.

Use most applicable Labour Operation from Canadian Labour Time Guide and Claim .7 Hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.