HOOD WOBBLES WHEN OPEN DUE TO LOOSE HINGE PIVOT BOLTS. Buick Skyhawk 1989

For 1990-2009 cars

# HOOD WOBBLES WHEN OPEN DUE TO LOOSE HINGE PIVOT BOLTS

#### MODELS AFFECTED: 1988-1989 SKYHAWK

Some 1988-1989 Skyhawks may have hood bolts that have insufficient loctite and could loosen. This will allow the hood to have a loose wobbly feel when opened. This condition has been corrected in production at the following VIN breakpoints: 1G4JSS110KK421521, 4/18/89.

To repair this condition, install new hinge pivot bolts, part number 22548097. Parts are currently available through GMSPO. Refer to the illustration for identification (the new bolt has a hex head).

#### WARRANTY INFORMATION

Labor Operation Number: T4654 Labor Time: 0.4 hrs both Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.