POOR A/C PERFORMANCE OR LEAK (MAYBE LEAK FROM HOSE). Buick Skyhawk 1986

For 1990-2009 cars

# POOR A/C PERFORMANCE OR LEAK (MAYBE LEAK FROM HOSE)

#### MODELS AFFECTED: 1986 BUICK SKYHAWKS WITH 1.8L OHC TURBO ENGINES (VIN CODE J)

Some 1986 Buick Skyhawks equipped with the LA5 engine (1.8L OHC turbo) and C60 air conditioning may experience a leaking A/C suction/discharge hose assembly due to the hoses coming in contact with each other.

Check hose assembly for abrasion or rub through and replace if necessary with Part Number 10040317.

#### NOTICE: Hose assembly should have a 25 m (I inch) clearance between the hoses, and if necessary, bend the pipes to assure this clearance. Refer to illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.