RACK & PINION 'SHORT GEAR' FOR FRONT WHEEL-DRIVE MODELS. Buick Skyhawk 1983

For 1990-2009 cars

# RACK & PINION 'SHORT GEAR' FOR FRONT WHEEL-DRIVE MODELS

#### Models Affected: 1982-1984 Skyhawk, Skylark, Century & 1985 Electra

"Short Gear" rack and pinion assemblies are available for service replacementt. The short gear is a complete gear assembly except for the following:

End Takeoff Gear Center Takeoff Gear ---------------- ------------------- 1. Inner and outer tie rod assemblies 1. Inner and outer tie rod assemblies

2. Tie rod boots

3. Breather tube

4. Attachment hardware

Boot clamps are included with the short gear.

Use of the short gear is recommended when the expense of individual parts and required labor necessary to service a rack and pinion assembly would exceed the expense of installing the short gear assembly. The short gear incorporates all product improvements made since 1982.

Refer to the chassis service manual for informatuin on parts transfer or R&R procedures.

#### CAUTION:

Failure to disconnect the intermediate shaft from the rack and pinion stub shaft prior to lowering the cradle can result in damage to the steering gear and/or intermediate shaft. Operation of the vehicle with this damage can cause loss of steering control which could result in personal injury.

#### REPLACEMENT APPLICATION

Service Short Year & Model Gear Part No. ------------ ------------- 1982-84 Century & Skylark 7846792 1982-84 Century & Skylark with F41 Suspension 7846779 1982-84 Skyhawk 7847127 1985 Electra 7846780

LABOR TIME ALLOWANCE: ---------------------- Operation Labor Usage Year/Model Number Time ------ ----------- ------ ----- Automatic Transaxle 1982 Century, Skylark E9730 1.7 Automatic Transaxle 1983 Century, Skylark E9730 2.1 Automatic Transaxle 1984 Century, Skylark E9730 2.2 Manual Transaxle 1982-84 Skylark E9730 1.9 Manual/Automatic Transaxle 1982-84 Skyhawk E9730 2.3 Automatic Transaxle 1985 Electra E9730 2.1

Use applicable trouble code and failed part number.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.