For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cooling System

- Engine Cooling, 2.4L

9.8 liters

10.4 quarts

- Engine Cooling, 3100

12.4 liters

13.1 quarts

Engine Crankcase

- With filter

3.78 liters

4.0 quarts

Fuel Tank | 57.5 liters | 15.2 gallons
Transaxle

- 3T40 Transaxle (Bottom Pan Removal

3.8 liters

4.0 quarts

- 3T40 Transaxle (Overhaul)

6.6 liters

7.0 quarts

- 3T40 Transaxle (Dry)

8.5 liters

9.0 quarts

- 4T60E Transaxle (Bottom Pan Removal)

5.7 liters

6.0 quarts

- 4T60E Transaxle (Complete Overhaul)

7.6 liters

8.0 quarts

- 4T60E Transaxle (Dry)

9.5 liters

10.0 quarts

- Manual Transaxle

1.9 liters

2.0 quarts