For 1990-2009 cars

# INFO ON NEW SPEC TOOL J28467- 330 ENG SUPPORT FIXTURE ADAPT

#### SUBJECT: 1992 "N" CAR WITH 3.3L (VIN N) RPO LG7 AND AUTOMATIC TRANSMISSION

#### SERVICE INFORMATION:

- USE J 28467-330 ENGINE SUPPORT FIXTURE ADAPTER FOR SUPPORTING THE ENGINE WHEN SERVICING ENGINE/TRANSMISSION COMPONENTS.

- TO USE J 28467-330 ADAPTER: 1. LOOSEN PILOT BOLTS ON BOTH ENDS OF ADAPTER. 2. PLACE PILOT BOLTS IN HOLES IN TIE BAR, REFER TO FIGURE 1 - VIEW B. 3. TIGHTEN PILOT BOLTS. 4. ATTACH J 28467-A TO STRUT TOWERS AND PLACE THE LEG OF J 28467-A ON ADAPTER AS SHOWN IN FIGURE 1. 5. ATTACH ENGINE SUPPORT HOOKS TO ENGINE SUPPORT FIXTURE AND ENGINE LIFT HOOKS.

#### NOTICE: FAILURE TO USE J 28467-330 IN CONJUNCTION WITH J 28467-A TO SUPPORT ENGINE MAY CAUSE DAMAGE TO BODY OR ENGINE COMPONENTS.

- J28467-330 ENGINE SUPPORT FIXTURE ADAPTER TOOL IS SCHEDULED TO BE DELIVERED TO DEALERS ON 7-1-92.

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1992 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.