For 1990-2009 cars

## Rear Compartment Courtesy Lamp Replacement Pontiac

### Removal Procedure

1. Open the rear compartment.
2. Release the tabs that retain the rear compartment lamp cover.
3. Release the tangs from the bulb.
4. Remove the bulb.

### Installation Procedure

1. Install the bulb into the socket. Snap the bulb fully into place.
2. Install the lamp cover.
3. Close the rear compartment.

## Rear Compartment Courtesy Lamp Replacement Buick/Oldsmobile

### Removal Procedure

1. Push inward on the bulb.
2. Rotate the bulb counter-clockwise.
3. Remove the bulb from the socket.

### Installation Procedure

1. Insert the bulb into the socket.
2. Push inward on the bulb.
3. Rotate the bulb clockwise.