For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check for vehicle overloading. Is the vehicle overloaded? | -- | Remove excess weight. | Go to Step 2
2 | Check the condition of the strut dampeners, shock absorbers or mounting. Are the strut dampeners, shock absorbers or mounting worn? | -- | Go to Strut Assembly Replacement | Go to Step 3
3 | Check for an incorrect, broken or worn spring. Is the spring incorrect, broken or worn? | -- | Go to Strut, Strut Component and/or Spring Replacement in Front Suspension | System OK