For 1990-2009 cars

#### Convienence Center

Connector Part Information |

• | 12160707

• | 22-Way (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PNK | 539 | Fuse Output - Ignition 1 - Type III Fuse
2 | ORN | 140 | Fuse Output - Battery - Type III Fuse
3 | BRN | 27 | Hazard Flasher Output
4 | PPL | 16 | Turn Signal Flasher Output
5 | BLK | 150 | Ground
A | DK GRN /WHT | 817 | Vehicle Speed Signal - 4000 Pulses/Mile
B | -- | -- | Not Used
C | PPL | 16 | Turn Signal Flasher Output
D | BRN | 9 | Park Lamp Feed
E | LT GRN | 80 | Key Reminder Switch Signal
F | LT BLU | 292 | Rear Defogger Switch Signal - Primary
G | LT BLU | 395 | Door Handle Switch Signal - Right Front
H | LT GRN/BLK | 394 | Door Handle Switch Signal - Left Front
J | ORN/BLK | 17866 | Transaxle Park/Neutral Signal
K | BLK/WHT | 238 | Seat Belt Switch Signal
L | PPL | 681 | Rear Defogger Switch Signal - Secondary
M | PNK | 39 | Fuse Output - Ignition 1 - Type III Fuse
N | BRN | 994 | Automatic Door Lock/Unlock Power Feed
P | LT BLU | 195 | Power Door Lock Relay Feed - Lock Coil
R | ORN | 1640 | Fuse Output - Battery - Type III Fuse
S | BLK | 28 | Horn Relay Output - Coil
T | DK GRN | 29 | Horn Feed