For 1990-2009 cars

In order to overhaul, follow the sequence below.

1. Torque Converter Disassemble
2. Transmission Holding Fixture Assemble
3. Vacuum Modulator and Valve Disassemble
4. Reverse Servo Disassemble
5. Forward Servo Disassemble
6. Bottom Pan and Filter Disassemble
7. Oil Filter Inspection
8. Accumulator Assembly, 2-1 Band Servo Disassemble
9. Control Valve Body Cover and Gasket Disassemble
10. Wiring Harness Disassemble
11. Oil Pump Disassemble
12. Control Valve Body and Spacer Plate Disassemble
13. Oil Pump Drive Shaft Removal
14. Vehicle Speed Sensor Disassemble
15. Output Shaft Disassemble
16. Front Differential Carrier End Play Check
17. Manual Valve Link and Fluid Dam Removal
18. Case Cover and Gaskets Disassemble
19. 4th Clutch Components Disassemble
20. Drive Link Stretch Check
21. Drive Sprocket, Driven Sprocket, and Drive Link Disassemble
22. Driven Sprocket Support Disassemble
23. 2nd Clutch and Input Clutch Removal
24. Reverse Band Disassemble
25. Reverse Reaction Drum Removal
26. Input Clutch Housing End Play Check
27. Case Extension Housing Disassemble
28. Differential Carrier Components Disassemble
29. Input and Reaction Carrier Disassemble
30. Reaction Sun Gear and Manual 2-1 Band Disassemble
31. 1-2 Support Drum and Forward Band Disassemble
32. Differential Carrier Internal Gear Disassemble
33. Park System Components Disassemble
34. Case Assembly Inspection
35. Case Components Disassemble
36. Case Components Assemble
37. Torque Converter Fluid Seal Removal
38. Drive Sprocket Support Disassemble
39. Drive Sprocket Support Assemble
40. Torque Converter Oil Seal Assemble
41. Park System Components Assemble
42. Differential Carrier Internal Gear Assemble
43. Differential Carrier Inspection
44. Differential Carrier Disassemble
45. Differential Carrier Assemble
46. Vehicle Speed Sensor Reluctor Wheel Disassemble
47. Vehicle Speed Sensor Reluctor Wheel Assemble
48. Differential Carrier Components Assemble
49. Case Extension Assemble
50. Input Clutch Housing End Play Tool Assemble
51. Forward Band Assemble
52. 1-2 Support Roller Clutch Disassemble
53. 1-2 Support Roller Clutch Assemble
54. 1-2 Support Roller Clutch Functional Check
55. 1-2 Support Drum Assemble
56. 2-1 Manual Band Assemble
57. Reaction Sun Gear and Drum Assemble
58. Input and Reaction Carrier Pinion End Play Check
59. Input and Reaction Carrier Assemble
60. Reverse Reaction Drum Assemble
61. Input and Third Sprag Clutches Disassemble
62. Input and Third Sprag Clutches Assemble
63. Input and Third Sprag Clutches Functional Check
64. Input Clutch and Third Clutch Disassemble
65. Input Clutch Housing Assembly Inspection
66. Input Clutch Housing Retainer and Ball Disassemble
67. Input Clutch Housing Retainer and Ball Assemble
68. Input Clutch and Third Clutch Assemble
69. Input Clutch and Third Clutch Functional Air Check
70. Input Clutch Housing Oil Seal Rings Assemble
71. Input Clutch Housing and Sprag Clutches Assemble
72. Input Clutch Housing End Play Check
73. 2nd Clutch Disassemble
74. 2nd Clutch Housing Assembly Inspection
75. Second Clutch Housing Retainer/Ball Disassemble
76. Second Clutch Housing Retainer/Ball Assemble
77. 2nd Clutch Assemble
78. Reverse Band Assemble
79. Driven Sprocket Support Components Disassemble
80. Driven Sprocket Support Components Inspection
81. Driven Sprocket Support Bearing Disassemble
82. Driven Sprocket Support Bearing Assemble
83. Driven Sprocket Support Components Assemble
84. 4th and 2nd Clutch Functional Air Check
85. Second, Input, and Sprag Clutches Assemble
86. Driven Sprocket Support Assemble
87. Drive Sprocket and Turbine Shaft Disassemble
88. Drive Sprocket and Turbine Shaft Assemble
89. Drive and Driven Sprocket Components Assemble
90. 4th Clutch Components Assemble
91. Case Cover Components Disassemble
92. Case Cover Components Inspection
93. Case Cover Bearing Disassemble
94. Case Cover Bearing Assemble
95. Drive Axle Oil Seal Removal - Left Side
96. Drive Shaft Oil Seal Assemble - Left Side
97. Case Cover Components Assemble
98. Case Cover and Gaskets Assemble
99. Manual Valve Link and Fluid Dam Assemble
100. Differential Carrier End Play Check
101. Output Shaft Bearing Disassemble
102. Output Shaft Assemble
103. Right Drive Shaft Oil Seal Disassemble
104. Right Drive Shaft Oil Seal Assemble
105. Vehicle Speed Sensor Assemble
106. Control Valve Body Clean
107. Control Valve Body Inspection
108. Control Valve Body Disassemble
109. Control Valve Body Assemble
110. Oil Pump Shaft Bearing Disassemble
111. Oil Pump Shaft Bearing Assemble
112. Oil Pump Drive Shaft Assemble
113. Control Valve Body and Spacer Plate Assemble
114. Transmission Fluid Pump Disassemble
115. Transmission Fluid Pump Assemble
116. Wiring Harness Assemble
117. Control Valve Body and Gasket Assemble
118. Thermo Element Adjustment
119. 2-1 Manual Band Servo Disassemble
120. 2-1 Manual Band Servo Assemble
121. Accumulator Components Disassemble
122. Accumulator Components Assemble
123. Accumulator Assembly, 2-1 Band Servo Assemble
124. Oil Pan and Filter Assemble
125. Forward Band Servo Components Disassemble
126. Forward Band Servo Assemble
127. Reverse Band Servo Components Disassemble
128. Reverse Band Servo Assemble
129. Vacuum Modulator Inspection
130. Vacuum Modulator and Valve Assemble
131. Transmission Holding Fixture Disassemble
132. Torque Converter Inspection
133. Torque Converter Assemble